>> MIB - Management Information Base
>> Table: ipSifAliasAddressTable - (.1.3.6.1.4.1.272.4.5.28.1)
Description: Contents a Stateful inspection Firewall description for a alias Name
ipSifAliasAddressTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Alias | DisplayString | RW
.3 | Address | IpAddress | RW
.4 | Mask | IpAddress | RW
.5 | Interface | INTEGER | RW
.6 | Mode | ENUM | D
.7 | Range | INTEGER | RW
.8 | Group | INTEGER | RW
.9 | ValueType | ENUM | RW
.10 | Value | InetAddress | RW
.11 | Length | INTEGER | RW
Index
The Index for the address alias
Alias
Alias Name for the Address Entry Length: 0 to 255
Address
The ip-address for the Alias
Mask
The ip Mask for the Alias
Interface
The interface index for the alias
Mode
Address or Interface Mode Enumerations: interface (1) address (2) range (3) delete (4)
Range
The ip Range for the Alias Range: 0 to 65535
Group
For values greater than zero this entry determines the IP address group this entry belongs to, see also ipSifAliasAddressGroupId
ValueType
Specifies the type of the 'ipSifAliasAddressValue', IPv4, IPv6, or qdn Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Value
Contains the address value according the specified type Length: 0 to 255
Length
The length of the Prefix / Mask Range: 0 to 128

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH