>> MIB - Management Information Base
>> Table: voipProviderTable - (.1.3.6.1.4.1.272.4.33.1.1)
Description: Contains parameters common to all VoIP provider types.
voipProviderTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | AdminStatus | ENUM | D
.3 | OperStatus | ENUM | R
.4 | Descr | DisplayString | RW
.5 | Domain | DisplayString | RW
.6 | Port | INTEGER | RW
.7 | Type | ENUM | RW
.8 | Account | DisplayString | RW
.9 | Pwd | OCTET STRING | RW
.20 | ProfileNo | INTEGER | R
Index
Unique index for referencing this provider entry. Range: 1 to 65535
AdminStatus
Administrative status for this provider instance. Enumerations: enable (1) disable (2) delete (3)
OperStatus
Current operative state of provider. Enumerations: down (11) dormant (12) trying (13) register (14) authenticate (15) up (16) failed (17) blocked (18) disable (19)
Descr
User defined description of this entry. Length: 0 to 255
Domain
IP address or fully qualified domain name (FQDN) of this VoIP provider instance. Length: 0 to 255
Port
Optional destination port of this VoIP provider (e.g 5060 for SIP or 1720 for H.323), if set to '0' this port will be selected otherwise (e.g. in case of SIP via DNS lookup for a SRV record). Range: 0 to 65535
Type
Type of provider (H.323, MGCP, SIP). Currently only SIP is implemented. In case of type SIP a further (automatically added) voipSipProviderTable with the same table index defines further variables for SIP provider. Enumerations: unknown (1) h323 (2) mgcp (3) sip (4)
Account
Optional user name for login to provider (only if given). Length: 0 to 64
Pwd
Password or private key for login to provider (only if given). Length: 0 to 64
ProfileNo
This variable is only used internally and managed by TR069 daemon. An entry gets assigned to a VoIP Profile by it. Profile number 1 means that entry isn't modifiable by GUI. Profile 3 is even not not shown in GUI and gets only used if no other provider entry is available. A value of 0 means 'any other profile'

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH