>> MIB - Management Information Base
>> Table: ip6RelayTable - (.1.3.6.1.4.1.272.4.5.100.1.7.1)
Description: Each entry contains one IPv6 address to `physical' address equivalence.
ip6RelayTable
OID | Name | Type | Access
.1 | IfIndexV6 | InterfaceIndexOrZero | RC
.2 | Descr | DisplayString | RC
.3 | IfIndexV4 | InterfaceIndexOrZero | RC
.4 | Type | ENUM | D
.5 | LocalAddress | InetAddressIPv6 | RC
.6 | RemoteAddress | InetAddressIPv6 | RC
.7 | Mtu | INTEGER | RC
.8 | POP | InetAddressIPv4 | RC
.9 | Interval | INTEGER | RC
.10 | Secret | DisplayString | RC
.11 | TICUser | DisplayString | RC
.12 | TICSecret | DisplayString | RC
.13 | TICTunnel | DisplayString | RC
.14 | TICHost | DisplayString | RC
.15 | UsedLocalAddress | InetAddressIPv6 | R
.16 | UsedRemoteAddress | InetAddressIPv6 | R
.17 | UsedMtu | INTEGER | R
.18 | UsedPOP | InetAddressIPv4 | R
.19 | UsedSrc | InetAddressIPv4 | R
.20 | UsedInterval | INTEGER | R
.21 | UsedSecret | DisplayString | R
.22 | OperStatus | ENUM | R
IfIndexV6
Unique Identifier for this entry Range: 0 to 2147483647
Descr
Description or name of this entry. Length: 0 to 255
IfIndexV4
Specifies the associated IPv4 interface for this relay. Range: 0 to 2147483647
Type
Type of the tunnel. Enumerations: stf (1) stf-tic (2) stf-he (3) delete (16)
LocalAddress
Assigned local IPv6 endpoint address Length: 16 to 16
RemoteAddress
Remote IPv6 endpoint address Length: 16 to 16
Mtu
Mtu value for this tunnel. Range: 1280 to 4095
POP
IPv4 address for the relay gateway. Length: 4 to 4
Interval
Schedule interval for heartbeats.
Secret
Password or authentication phrase for heartbeats. Length: 0 to 255
TICUser
TIC protocol user name. Length: 0 to 255
TICSecret
TIC protocol password. Length: 0 to 255
TICTunnel
TIC tunnel ID. Length: 0 to 255
TICHost
TIC server address. Length: 0 to 255
UsedLocalAddress
Assigned local IPv6 address. Length: 16 to 16
UsedRemoteAddress
Assigned remote IPv6 address. Length: 16 to 16
UsedMtu
Mtu value for this tunnel. Range: 1280 to 4095
UsedPOP
IPv4 address of the associated relay gateway. Length: 4 to 4
UsedSrc
The local IPv4 address used for this tunnel. Length: 4 to 4
UsedInterval
Schedule interval for the heartbeats. Range: 0 to 3600
UsedSecret
TIC server address. Length: 0 to 255
OperStatus
The current operational status of this tunnel. Enumerations: up (1) down (2) update (3) authenticate (4) failed (5)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH