>> MIB - Management Information Base
>> Table: ip6CfgGlobals - (.1.3.6.1.4.1.272.4.5.100.1.1)
ip6CfgGlobals
OID | Name | Type | Access
.1 | Local | InetAddressIPv6 | RW
.2 | DUID | OCTET STRING | R
Local
The Locally Assigned Global Id for the locally assigned Prefix. Length: 16 to 16
DUID
The locally unique DUID used by internal DHCPv6-client and server (see 9, 22.2, 22.3 of RFC-3315).

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH