>> MIB - Management Information Base
>> Table: ip6PrefixTable - (.1.3.6.1.4.1.272.4.5.100.2.3.1)
Description: An interface entry containing objects of a particular IPv6 address prefix.
ip6PrefixTable
OID | Name | Type | Access
.1 | Id | Unsigned32 | R
.2 | IfIndex | InterfaceIndexOrZero | R
.3 | Prefix | InetAddressIPv6 | R
.4 | Length | INTEGER | R
.5 | OnLinkFlag | ENUM | R
.6 | AutonomousFlag | ENUM | R
.7 | AdvValidLifetime | Unsigned32 | R
.8 | AdvPreferredLifetime | Unsigned32 | R
.9 | NextHop | InetAddressIPv6 | R
.10 | Type | ENUM | R
.11 | Age | TimeStamp | R
.12 | OperStatus | ENUM | R
.13 | Slaac | ENUM | R
Id
A unique non-zero value identifying the particular IPv6 prefix.
IfIndex
A unique non-zero value identifying the particular IPv6 interface (or relay) index. Range: 0 to 2147483647
Prefix
The prefix associated with the this interface. Length: 16 to 16
Length
The length of the prefix (in bits). Range: 0 to 128
OnLinkFlag
true: Prefix can be used for on-link determination Enumerations: true (1) false (2)
AutonomousFlag
true: stateless configuration possible false: no autoconfiguration possible Enumerations: true (1) false (2)
AdvValidLifetime
The value in seconds the prefix will be remain valid.
AdvPreferredLifetime
The length in seconds the prefix will be remain preferred.
NextHop
The prefix associated with the this interface. Length: 16 to 16
Type
The working mode of the prefix. Enumerations: dynamic (1) static (2)
Age
The timestamp of last update of the prefix.
OperStatus
The current status of the prefix up prefix is valid down prefix is not valid Enumerations: up (1) down (2)
Slaac
SLAAC method, in conjunction with the ip6PrefixAutonomousFlag this setting determines the address format which should be the result of the address autoconfiguration procedure eui64 EUI-64-Identifier according RFC 4291 privacy-ext Privacy Extensions according RFC 4941 none no SLAAC will be performed Enumerations: eui64 (1) privacy-ext (2) none (3)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH