>> MIB - Management Information Base
>> Table: ipSifExpectTable - (.1.3.6.1.4.1.272.4.5.35.1)
Description: Contains expected but not yet established essions.
ipSifExpectTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Source | IpAddress | R
.3 | Destination | IpAddress | R
.4 | Protocol | ENUM | D
.5 | SourcePort | INTEGER | R
.6 | DestPort | INTEGER | R
.7 | Priority | ENUM | R
.8 | ClassId | INTEGER | R
.9 | IfIndex | INTEGER | R
.10 | SrcType | ENUM | R
.11 | Src | InetAddress | R
.12 | DstType | ENUM | R
.13 | Dst | InetAddress | R
Index
This field is used for SIF-internal signalling and stores the index for the expected session for later matching.
Source
The source-IP-address for the expected session. A value of 0 means ANY source-address.
Destination
The destination-IP-address for the expected session. A value of 0 means ANY destination-address.
Protocol
The protocol of the expected session. Enumerations: icmp (1) igmp (2) ip (4) tcp (6) udp (17) delete (255)
SourcePort
The source-port-number of the expected session. A value of 0 means ANY source-port-number.
DestPort
The destination-port-number of the expected session. A value of 0 means ANY destination-port-number.
Priority
Defines the QoS-priority/policy to be used for the expected SIF-session. Enumerations: default (1) low-latency (2) high (3) medium (4) low (5)
ClassId
Internal ID for mapping SIF-policy to QoS-policy. Default-value of 0 means NOT SPECIFIED. Range: 1 to 255
IfIndex
Interface-index for which the session is expected. A value of 0 means ANY interface-index.
SrcType
The type of the destination IP adresses, ipv4 or ipv6 Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Src
The source-IP/IPv6-address for the expected session. A value of 0.0.0.0 or :: means ANY source-address. Length: 0 to 255
DstType
The type of the destination IP adresses, ipv4 or ipv6 Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Dst
The destination-IP/IPv6-address for the expected session. A value of 0.0.0.0. or :: means ANY destination-address. Length: 0 to 255

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH