>> MIB - Management Information Base
>> Table: mpsSysTimer - (.1.3.6.1.4.1.272.4.53.1.2)
mpsSysTimer
OID | Name | Type | Access
.1 | CFNR | INTEGER | RW
.2 | ExternalDoorIntercomTimeout | ENUM | RW
.3 | RecallTimeout | INTEGER | RW
.4 | RecallBusyTimeout | INTEGER | RW
.5 | DirectCall | INTEGER | RW
.6 | ExternalAlarmCallTimeout | ENUM | RW
.7 | DropCallNoReply | INTEGER | RW
.8 | DTMFAck | INTEGER | RW
.9 | DiallingBreakGSM | INTEGER | RW
.10 | SystemPark | INTEGER | RW
CFNR
This variable contains the length of timer in seconds of call forwarding no reply. Range: 1 to 99
ExternalDoorIntercomTimeout
This variable contains the length of timer in seconds. Enumerations: off (1) s60 (2) s120 (3) s180 (4) s240 (5) s300 (6)
RecallTimeout
This variable contains the length of timer in seconds. Range: 10 to 179
RecallBusyTimeout
This variable contains the length of timer in seconds. Range: 10 to 600
DirectCall
This variable contains the length of timer in seconds. Range: 1 to 30
ExternalAlarmCallTimeout
This variable contains the length of timer. For further implementations this global variable (that never shown via GUI until now) is obsolete und swapped to the mpsAlarmInputTable. Enumerations: off (1) s60 (2) s120 (3) s180 (4) s240 (5) s300 (6)
DropCallNoReply
This variable contains the length of timer in seconds. Range: 1 to 120
DTMFAck
This variable contains the length of timer in seconds. Range: 5 to 60
DiallingBreakGSM
This variable contains the length of timer in seconds. Range: 0 to 5
SystemPark
This variable contains the length of timer in seconds. Range: 10 to 600

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH