>> MIB - Management Information Base
>> Table: ip6DhcpClientPrefixTable - (.1.3.6.1.4.1.272.4.5.100.4.13.1)
Description: Currently assigned prefixes.
ip6DhcpClientPrefixTable
OID | Name | Type | Access
.1 | Value | InetAddressIPv6 | R
.2 | Length | INTEGER | R
.3 | DUID | OCTET STRING | R
.4 | PoolId | INTEGER | R
.5 | IAID | Unsigned32 | R
.6 | PrefLifetime | Unsigned32 | R
.7 | ValidLifetime | Unsigned32 | R
.8 | FwdIfIndex | InterfaceIndex | R
.9 | FwdAddress | InetAddressIPv6 | R
.10 | Age | TimeStamp | R
Value
Assigned prefix. Length: 16 to 16
Length
Length of assigned prefix. Range: 0 to 64
DUID
DUID of related DHCPv6-client (see 9 and 22.2 of RFC-3315).
PoolId
'Id' value of related 'ip6DhcpPrefixPool' entry.
IAID
IAID of related IA_PD (see 9 of RFC-3633).
PrefLifetime
'Preferred lifetime' in seconds of assigned prefix (see 10 of RFC-3633).
ValidLifetime
'Valid lifetime' in seconds of assigned prefix (see 10 of RFC-3633).
FwdIfIndex
Together with 'ip6DhcpClientPrefixFwdAddress', tells next hop for forwarding IPv6-frames targeted to this prefix. This info equals to target of related IA_PD option. See also description for 'ip6DhcpPrefixPoolAutoRoutePrio'. Warning: Do not confuse forwarding-interface (chosen by server) with on-link-interface (chosen by client). Range: 1 to 2147483647
FwdAddress
See description for 'ip6DhcpClientPrefixFwdIfIndex'. Length: 16 to 16
Age
Age of this prefix-entry.

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH