>> MIB - Management Information Base
>> Table: sysConfigAdmin - (.1.3.6.1.4.1.272.4.17.9.1)
sysConfigAdmin
OID | Name | Type | Access
.1 | LedMode | ENUM | RW
.2 | TftpBootLocalIpAddr | IpAddress | RW
.3 | TftpBootServerIpAddr | IpAddress | RW
.4 | TftpBootFile | DisplayString | RW
.5 | AutoTftpBoot | ENUM | RW
.6 | FunctionBootState | ENUM | RW
.7 | OperationMode | ENUM | R
LedMode
The LED mode of the system: normal : LEDs work normal, minimal : only Status-LED flashes once in a second, off := LEDs are off. Enumerations: normal (1) minimal (2) off (3)
TftpBootLocalIpAddr
Local IP address for TFTP boot.
TftpBootServerIpAddr
IP address of TFTP sever.
TftpBootFile
Name of the TFTP boot file. Length: 0 to 255
AutoTftpBoot
Indicates whether the device tries to boot the image from TFTP server. If this fails it will stay in the bootmonitor mode. Enumerations: no (1) yes (2)
FunctionBootState
This variable configures how the initial value of sysStatFunctionState is determined: last : use value out of NVRAM on : set to on off : set of off. Enumerations: last (1) on (2) off (3)
OperationMode
This variable indicates the operation mode of the device how it will come up on next system start. If any voice functionality is integrated it can be either mgw(1) for Media GateWay functionality of pbx(2) for a full-fledged telephone system. For systems w/o voice functionality the variable has value plain(0). Enumerations: plain (0) mgw (1) pbx (2)

MIB Reference to Software Version 10.1.21 generated on 2016/12/23. Provided by webmaster@bintec-elmeg.com Copyright ©2016 by bintec elmeg GmbH