>> MIB - Management Information Base
>> Table: auxMobileOperatorTable - (.1.3.6.1.4.1.272.4.41.3.1.13.1)
Description: A single auxMobileOperatorTable entry.
auxMobileOperatorTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | ID | INTEGER | R
.3 | AccessType | ENUM | R
.4 | Status | ENUM | R
.5 | Name | DisplayString | R
IfIndex
The index of the corresponding tty interface.
ID
The international unique ID of the network operator.
AccessType
The Access Type the modem actually registers on. Normally the `edge' or `hs*pa' Access Types aren't provided in detail by the operator. Enumerations: unknown (1) gsm (2) compact-gsm (3) umts (4) gsm-edge (5) umts-hsdpa (6) umts-hsupa (7) umts-hspa (8)
Status
The registration status depending on the network operator. The following states can occur: - unknown(1) -- no idea - available(2) -- registration possible - current(3) -- successfully registered - forbidden(4) -- no roaming possible Enumerations: unknown (1) available (2) forbidden (4)
Name
The name of the network operator. Range: 0 to 60

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH