>> MIB - Management Information Base
>> Table: wlanIfFeatureTable - (.1.3.6.1.4.1.272.4.46.23.1)
Description: This table lists all feature of a wireless card. The supported features depends on the vendor and wireless chipset.
wlanIfFeatureTable
OID | Name | Type | Access
.1 | WlanIf | INTEGER | R
.2 | OperatingBands | BITS | R
.3 | AntennaDiversity | ENUM | R
.4 | TxPowerMin | INTEGER | R
.5 | TxPowerMax | INTEGER | R
.6 | TxPowerFixedStepsList | DisplayString | R
.7 | FrameCompression | ENUM | R
.8 | FrameConcatenation | ENUM | R
.9 | PiggybackAck | ENUM | R
.10 | DirectLink | ENUM | R
.11 | LinkDistance | ENUM | R
.12 | ShortRetries | ENUM | R
.13 | LongRetries | ENUM | R
.14 | FragThreshold | ENUM | R
.15 | CCAMode | ENUM | R
.16 | EdThreshold | ENUM | R
.17 | CWMin | ENUM | R
.18 | CWMax | ENUM | R
.19 | RxLifetime | ENUM | R
.20 | TxLifetime | ENUM | R
.21 | SkipModes | BITS | R
WlanIf
Wireless card interface index the table belongs.
OperatingBands
This variable says which bands the wireless card supports. Default is 2.4 and 5 GHZ. Enumerations: band24 (0) band5 (1) band58 (2)
AntennaDiversity
This variable says which kind of antenna diversity the wireless card supports. Default is none. Enumerations: none (0) rx (1) tx (2) rx-tx (3)
TxPowerMin
The minimal value of the TX power the wireless card supports. Range: 0 to 30
TxPowerMax
The maximal value of the TX power the wireless card supports. Range: 0 to 30
TxPowerFixedStepsList
This variable shows the available TX Power values in dBm seperated by commas. Range: 0 to 255
FrameCompression
This variable says if the wireless card supports frame compression or not. Default is false. Enumerations: true (1) false (2)
FrameConcatenation
This variable says if the wireless card supports frame concatination or not. Default is false. Enumerations: true (1) false (2)
PiggybackAck
This variable says if the wireless card supports piggyback ACKs or not. Default is false. Enumerations: true (1) false (2)
DirectLink
This variable says if the wireless card supports direct links or not. Default is false. Enumerations: true (1) false (2)
LinkDistance
This variable says if the wireless card supports a configurable link distance or not. Default is false. Enumerations: true (1) false (2)
ShortRetries
This variable says if the wireless card supports the configuration of the short retry value or not. Default is false. Enumerations: true (1) false (2)
LongRetries
This variable says if the wireless card supports the configuration of the long retry value or not. Default is false. Enumerations: true (1) false (2)
FragThreshold
This variable says if the wireless card supports the configuration of the fragmentation threshold value or not. Default is false. Enumerations: true (1) false (2)
CCAMode
This variable says if the wireless card supports the configuration of the CCA mode or not. Default is false. Enumerations: true (1) false (2)
EdThreshold
This variable says if the wireless card supports the configuration of the energy detection threshold value or not. Default is false. Enumerations: true (1) false (2)
CWMin
This variable says if the wireless card supports the configuration of the minimal contention window or not. Default is false. Enumerations: true (1) false (2)
CWMax
This variable says if the wireless card supports the configuration of the maximal contention window or not. Default is false. Enumerations: true (1) false (2)
RxLifetime
This variable says if the wireless card supports the configuration of the receive packet lifetime or not. Default is false. Enumerations: true (1) false (2)
TxLifetime
This variable says if the wireless card supports the configuration of the transmit packet lifetime or not. Default is false. Enumerations: true (1) false (2)
SkipModes
This variable says which modes of the WlanIfSkipChannels the wireless card supports. Default is client24ghz. Enumerations: ap24ghz (0) ap5ghz (1) client24ghz (2) client5ghz (3)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH