>> MIB - Management Information Base
>> Table: ipLoadBIfTable - (.1.3.6.1.4.1.272.4.5.41.1)
Description: The ipLoadBIfTable contains parameters related to the IP session-based load balancing algorithm. Each entry defines a load balancing interface group member via it's unique interface index. Entries can only be added or deleted by the user. Creating entries: Entries are created by assigning a value to the ipLoadBIfIndex object. Deleting entries: Entries are removed by setting an entry's ipLoadBIfMode object to 'delete'.
ipLoadBIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | GroupId | INTEGER | RW
.3 | Ratio | INTEGER | RW
.4 | Mode | ENUM | D
.5 | ActAssignedSessions | Counter | R
.6 | TotAssignedSessions | Counter | R
.7 | ActLoad | INTEGER | R
.8 | ActDownLoad | INTEGER | R
.9 | ActUpLoad | INTEGER | R
Index
The unique interface index.
GroupId
The unique ID of the interface group which the interface specified by the variable ipLoadBIfIndex belongs to. Range: 0 to 99
Ratio
For statistical IP session distribution only, determines the fraction of of all sessions or bandwidth consumption of the whole group projected for this interface. Range: 0 to 100
Mode
Currently an auxiliary variable for the user to enable/ disable the associated interface for load balancing or to delete this entry. Enumerations: enabled (1) disabled (2) delete (10)
ActAssignedSessions
Number of distributed IP sessions to the associated interface since last configuration or status change of the interface group.
TotAssignedSessions
Number of distributed IP sessions to the associated interface since startup of the system or enabling the load balancing.
ActLoad
Current bandwidth consumption in bits per second.
ActDownLoad
Current bandwidth consumption (download) in bits per second.
ActUpLoad
Current bandwidth consumption (upload) in bits per second.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH