>> MIB - Management Information Base
>> Table: mpsCallThroughTable - (.1.3.6.1.4.1.272.4.53.4.5.1)
Description: This table contains the information of each call through entry.
mpsCallThroughTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | InTrunkGroup | TrunkGroupIndex | RW
.3 | InNumberIndex | SubscriberNumberIndex | RW
.4 | OutTrunkGroup | TrunkGroupIndex | RW
.5 | OutNumberIndex | SubscriberNumberIndex | RW
.6 | OutBundle | INTEGER | RW
.7 | Facilities | BITS | R
.8 | AdminStatus | ENUM | D
.9 | Option | ENUM | RW
Index
A unique value for each call through entry.
InTrunkGroup
A unique value for the incoming trunk group. Range: 1 to 65535
InNumberIndex
This value index of the incoming external msn.
OutTrunkGroup
A unique value for the outgoing trunk group. Range: 1 to 65535
OutNumberIndex
This value index of the outgoing external msn.
OutBundle
A unique value for the outgoing bundle.
Facilities
Special facilities of the call through entry. clip_sreening : sreen the incoming phone number. ars : use ars (automatic route selection) Enumerations: clip-sreening (0) ars (1)
AdminStatus
For enable, disable or delete. Enumerations: enable (1) disable (2) delete (3)
Option
This value contains the authorisation option for the calling party. clipscr -> only clip screening pin -> only pin check clipscrAndPin -> clip screening and pin check clipscrOrPin -> clip screening or pin check Enumerations: clipscr (1) pin (2) clipscrAndPin (3) clipscrOrPin (4)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH