>> MIB - Management Information Base
>> Table: voipProviderTable - (.1.3.6.1.4.1.272.4.33.1.1)
Description: Contains parameters common to all VoIP provider types.
voipProviderTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | AdminStatus | ENUM | D
.3 | OperStatus | ENUM | R
.4 | Descr | DisplayString | RW
.5 | Domain | DisplayString | RW
.6 | Port | INTEGER | RW
.7 | Type | ENUM | RW
.8 | Account | DisplayString | RW
.9 | Pwd | OCTET STRING | RW
Index
Unique index for referencing this provider entry. Range: 1 to 65535
AdminStatus
Administrative status for this provider instance. Enumerations: enable (1) disable (2) delete (3)
OperStatus
Current operative state of provider. Enumerations: down (11) dormant (12) trying (13) register (14) authenticate (15) up (16) failed (17) blocked (18) disable (19)
Descr
User defined description of this entry. Range: 0 to 255
Domain
IP address or fully qualified domain name (FQDN) of this VoIP provider instance. Range: 0 to 255
Port
Optional destination port of this VoIP provider (e.g 5060 for SIP or 1720 for H.323). Range: 1 to 65535
Type
Type of provider (H.323, MGCP, SIP). Currently only SIP is implemented. In case of type SIP a further (automatically added) voipSipProviderTable with the same table index defines further variables for SIP provider. Enumerations: unknown (1) h323 (2) mgcp (3) sip (4)
Account
Optional user name for login to provider (only if given). Range: 0 to 64
Pwd
Password or private key for login to provider (only if given). Range: 0 to 64

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH