>> MIB - Management Information Base
>> Table: hdsl2ShdslSpanConfProfileTable - (.1.3.6.1.4.1.272.4.35.1.1.10.1)
Description: Each entry corresponds to a single span configuration profile. Each profile contains a set of span configuration parameters. The configuration parameters in a profile are applied to those lines referencing that profile (see the hdsl2ShdslSpanConfProfile object). Profiles may be created/deleted only by the system.
hdsl2ShdslSpanConfProfileTable
OID | Name | Type | Access
.1 | ProfileName | DisplayString | R
.2 | WireInterface | ENUM | RW
.3 | MinLineRate | INTEGER | RW
.4 | MaxLineRate | INTEGER | RW
.6 | TransmissionMode | ENUM | RW
.10 | WorstCaseTargetMarginDown | INTEGER | RW
.12 | WorstCaseTargetMarginUp | INTEGER | RW
ProfileName
This object is the unique index associated with this profile. Entries in this table are referenced via the object hdsl2ShdslSpanConfProfile in Hdsl2ShdslSpanConfEntry. Range: 1 to 32
WireInterface
This object configures the two-wire or optional four-wire operation for SHDSL Lines. Enumerations: twoWire (1) fourWire (2) fourWireStandard (3) fourWireIMA (4) sixWire (5) sixWireIMA (6) eightWire (7) eightWireIMA (8) not-used (9) groupMember (10)
MinLineRate
This object configures the minimum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
MaxLineRate
This object configures the maximum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
TransmissionMode
This object specifies the regional setting for the SHDSL line: region1 - ITU-T G.991.2 Annex A region2 - ITU-T G.991.2 Annex B Enumerations: region1 (1) region2 (2) region1or2 (3)
WorstCaseTargetMarginDown
This object specifies the downstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: 0 to 65535
WorstCaseTargetMarginUp
This object specifies the upstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 21

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH