>> MIB - Management Information Base
>> Table: mpsArsCarrierTable - (.1.3.6.1.4.1.272.4.53.10.6.1)
Description: This table contains information for each Automatic Route Selection Carrier of the routing.
mpsArsCarrierTable
OID | Name | Type | Access
.1 | Index | CarrierIndex | RW
.2 | DisplayName | DisplayString | RW
.3 | Number | DisplayString | RW
.4 | NumberPresentation | ENUM | RW
.5 | RoutingMode | ENUM | RW
.6 | RoutingModeNumber | DisplayString | RW
.7 | RoutingAdminStatus | ENUM | D
Index
A unique index for each carrier.
DisplayName
This object specifies a Carrier description for the Autom. Route Selection functionality. The DiaplayName can be shown on the Systel Phones. Range: 0 to 20
Number
This object specifies the number inserted to select a special route (carrier). Range: 0 to 12
NumberPresentation
Enumerations: show (1) hide (2)
RoutingMode
A unique value for each day of the calendar. Set to delete to discard the whole entry. Enumerations: standard (1) bundle (2) msn (3)
RoutingModeNumber
This object specifies the bundle or internal msn depending on the selected RoutingMode. Range: 0 to 4
RoutingAdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH