>> MIB - Management Information Base
>> Table: wlanLinkTestHTStatsTable - (.1.3.6.1.4.1.272.4.46.19.1)
Description: The wlanLinkTestHTStatsTable contains additional statistical data about 802.11n HT frames for WDS links. Each entry corresponds to an wlanWDSTable entry. Entries cannot be added or deleted by the user.
wlanLinkTestHTStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | RxFramesMCS0 | Counter32 | R
.3 | RxFramesMCS1 | Counter32 | R
.4 | RxFramesMCS2 | Counter32 | R
.5 | RxFramesMCS3 | Counter32 | R
.6 | RxFramesMCS4 | Counter32 | R
.7 | RxFramesMCS5 | Counter32 | R
.8 | RxFramesMCS6 | Counter32 | R
.9 | RxFramesMCS7 | Counter32 | R
.10 | RxFramesMCS8 | Counter32 | R
.11 | RxFramesMCS9 | Counter32 | R
.12 | RxFramesMCS10 | Counter32 | R
.13 | RxFramesMCS11 | Counter32 | R
.14 | RxFramesMCS12 | Counter32 | R
.15 | RxFramesMCS13 | Counter32 | R
.16 | RxFramesMCS14 | Counter32 | R
.17 | RxFramesMCS15 | Counter32 | R
.18 | RxFramesRemoteMCS0 | Counter32 | R
.19 | RxFramesRemoteMCS1 | Counter32 | R
.20 | RxFramesRemoteMCS2 | Counter32 | R
.21 | RxFramesRemoteMCS3 | Counter32 | R
.22 | RxFramesRemoteMCS4 | Counter32 | R
.23 | RxFramesRemoteMCS5 | Counter32 | R
.24 | RxFramesRemoteMCS6 | Counter32 | R
.25 | RxFramesRemoteMCS7 | Counter32 | R
.26 | RxFramesRemoteMCS8 | Counter32 | R
.27 | RxFramesRemoteMCS9 | Counter32 | R
.28 | RxFramesRemoteMCS10 | Counter32 | R
.29 | RxFramesRemoteMCS11 | Counter32 | R
.30 | RxFramesRemoteMCS12 | Counter32 | R
.31 | RxFramesRemoteMCS13 | Counter32 | R
.32 | RxFramesRemoteMCS14 | Counter32 | R
.33 | RxFramesRemoteMCS15 | Counter32 | R
.34 | BandwidthLocal | ENUM | R
.35 | GuardIntervalLocal | ENUM | R
.36 | RSSI1Local | WlanRSSI | R
.37 | RSSI2Local | WlanRSSI | R
.38 | RSSI3Local | WlanRSSI | R
.39 | BandwidthRemote | ENUM | R
.40 | GuardIntervalRemote | ENUM | R
.41 | RSSI1Remote | WlanRSSI | R
.42 | RSSI2Remote | WlanRSSI | R
.43 | RSSI3Remote | WlanRSSI | R
IfIndex
The interface index of the corresponding bridge interface.
RxFramesMCS0
This attribute shows the number of HT data frames that were received at MCS 0.
RxFramesMCS1
This attribute shows the number of HT data frames that were received at MCS 1.
RxFramesMCS2
This attribute shows the number of HT data frames that were received at MCS 2.
RxFramesMCS3
This attribute shows the number of HT data frames that were received at MCS 3.
RxFramesMCS4
This attribute shows the number of HT data frames that were received at MCS 4.
RxFramesMCS5
This attribute shows the number of HT data frames that were received at MCS 5.
RxFramesMCS6
This attribute shows the number of HT data frames that were received at MCS 6.
RxFramesMCS7
This attribute shows the number of HT data frames that were received at MCS 7.
RxFramesMCS8
This attribute shows the number of data frames that were received at MCS 8.
RxFramesMCS9
This attribute shows the number of HT data frames that were received at MCS 9.
RxFramesMCS10
This attribute shows the number of HT data frames that were received at MCS 10.
RxFramesMCS11
This attribute shows the number of HT data frames that were received at MCS 11.
RxFramesMCS12
This attribute shows the number of HT data frames that were received at MCS 12.
RxFramesMCS13
This attribute shows the number of HT data frames that were received at MCS 13.
RxFramesMCS14
This attribute shows the number of HT data frames that were received at MCS 14.
RxFramesMCS15
This attribute shows the number of HT data frames that were received at MCS 15.
RxFramesRemoteMCS0
This attribute shows the number of HT data frames that were transmitted at MCS 0.
RxFramesRemoteMCS1
This attribute shows the number of HT data frames that were transmitted at MCS 1.
RxFramesRemoteMCS2
This attribute shows the number of HT data frames that were transmitted at MCS 2.
RxFramesRemoteMCS3
This attribute shows the number of HT data frames that were transmitted at MCS 3.
RxFramesRemoteMCS4
This attribute shows the number of HT data frames that were transmitted at MCS 4.
RxFramesRemoteMCS5
This attribute shows the number of HT data frames that were transmitted at MCS 5.
RxFramesRemoteMCS6
This attribute shows the number of HT data frames that were transmitted at MCS 6.
RxFramesRemoteMCS7
This attribute shows the number of HT data frames that were transmitted at MCS 7.
RxFramesRemoteMCS8
This attribute shows the number of data frames that were transmitted at MCS 8.
RxFramesRemoteMCS9
This attribute shows the number of HT data frames that were transmitted at MCS 9.
RxFramesRemoteMCS10
This attribute shows the number of HT data frames that were transmitted at MCS 10.
RxFramesRemoteMCS11
This attribute shows the number of HT data frames that were transmitted at MCS 11.
RxFramesRemoteMCS12
This attribute shows the number of HT data frames that were transmitted at MCS 12.
RxFramesRemoteMCS13
This attribute shows the number of HT data frames that were transmitted at MCS 13.
RxFramesRemoteMCS14
This attribute shows the number of HT data frames that were transmitted at MCS 14.
RxFramesRemoteMCS15
This attribute shows the number of HT data frames that were transmitted at MCS 15.
BandwidthLocal
This attribute shows the bandwidth the remote side used: 20 MHz (1) or 40 MHz (2). Enumerations: b20MHz (1) b40MHz (2)
GuardIntervalLocal
This attribute shows the length of the guard interval the remote side used: long (1) or short (2). Enumerations: long (1) short (2)
RSSI1Local
This attribute shows the received signal strength on the first receiver in dBm. Range: -110 to 0
RSSI2Local
This attribute shows the received signal strength on the second receiver in dBm. Range: -110 to 0
RSSI3Local
This attribute shows the received signal strength on the third receiver in dBm. Range: -110 to 0
BandwidthRemote
This attribute shows the bandwidth the local side used for transmitting: 20 MHz (1) or 40 MHz (2). Enumerations: b20MHz (1) b40MHz (2)
GuardIntervalRemote
This attribute shows the length of the guard interval the local side used for transmitting: long (1) or short (2). Enumerations: long (1) short (2)
RSSI1Remote
This attribute shows the received signal strength on the first receiver on the remote side in dBm. Range: -110 to 0
RSSI2Remote
This attribute shows the received signal strength on the second receiver on the remote side in dBm. Range: -110 to 0
RSSI3Remote
This attribute shows the received signal strength on the third receiver on the remote side in dBm. Range: -110 to 0

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH