>> MIB - Management Information Base
>> Table: mpsGroupModeTable - (.1.3.6.1.4.1.272.4.53.5.2.1)
Description: This table contains the information of each Mode of a group.
mpsGroupModeTable
OID | Name | Type | Access
.1 | Index | GroupIndex | RW
.2 | Number | GroupModeIndex | RW
.3 | Operation | ENUM | RW
.4 | RoutingType | ENUM | RW
.5 | CFUEnable | ENUM | RW
.6 | CFUTargetNumber | DisplayString | RW
.7 | CFUSourceIndex | ExtensionIndexOrZero | RW
.8 | BusyOnBusy | INTEGER | RW
.9 | CFNRTimer | INTEGER | RW
.10 | CFNRTargetGroup | GroupIndexOrZero | RW
.11 | AdminStatus | ENUM | D
Index
A unique value for each group Range: 1 to 99
Number
A unique value for each mode of a group. Range: 1 to 2
Operation
Signalling mode of the group. Enumerations: multicast (1) chainNoRepeat (2) chainRepeat (3) growing (4) chainNoRepeatWithMulticastTimer (5) chainRepeatWithMulticastTimer (6) maxIdle (7)
RoutingType
Additonal info for the signalling mode. standard(1) : standard routing busyOnBusy(2): check busy conditions Enumerations: standard (1) busyOnBusy (2)
CFUEnable
Extension group members are internals or an external Enumerations: true (1) false (2)
CFUTargetNumber
This external number will be called, if mpsGroupModeAssignment = external. Range: 0 to 20
CFUSourceIndex
The charge information will be stored for this extension. Range: 0 to 65535
BusyOnBusy
A second call is to be signaled to the team as a call waiting (standard), or whether the caller is to hear a busy signal (Busy On Busy).
CFNRTimer
This is the delay until rerouting starts.
CFNRTargetGroup
Group index for rerouting. Range: 0 to 99
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH