>> MIB - Management Information Base
>> Table: wlanStationTable - (.1.3.6.1.4.1.272.4.46.5.1)
Description: The wlanStationTable contains information relating to the clients currently associated to our access points. Each entry corresponds to an associated client station (STA). Entries cannot be added or deleted by the user. Creating entries: Entries are created by the system automatically when a new STA ia associated. Deleting entries: Entries are removed by the system whenever an associated STA is removed.
wlanStationTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Address | MacAddress | R
.3 | VSSIndex | INTEGER | R
.4 | State | ENUM | D
.5 | Security | ENUM | R
.6 | Node | ENUM | R
.8 | MSDUTx | Counter32 | R
.9 | MSDURx | Counter32 | R
.10 | BytesTx | Counter32 | R
.11 | BytesRx | Counter32 | R
.12 | Rate | WlanRate | R
.13 | Signal | WlanRSSI | R
.14 | Noise | WlanRSSI | R
.15 | ConnectTime | Counter32 | R
.16 | TimeoutTStamp | Counter32 | N
.17 | TimeoutCount | Counter32 | N
.30 | RxFrames54 | Counter32 | R
.31 | RxFrames48 | Counter32 | R
.32 | RxFrames36 | Counter32 | R
.33 | RxFrames24 | Counter32 | R
.34 | RxFrames18 | Counter32 | R
.35 | RxFrames12 | Counter32 | R
.36 | RxFrames11 | Counter32 | R
.37 | RxFrames9 | Counter32 | R
.38 | RxFrames6 | Counter32 | R
.39 | RxFrames5 | Counter32 | R
.40 | RxFrames2 | Counter32 | R
.41 | RxFrames1 | Counter32 | R
.42 | TxFrames54 | Counter32 | R
.43 | TxFrames48 | Counter32 | R
.44 | TxFrames36 | Counter32 | R
.45 | TxFrames24 | Counter32 | R
.46 | TxFrames18 | Counter32 | R
.47 | TxFrames12 | Counter32 | R
.48 | TxFrames11 | Counter32 | R
.49 | TxFrames9 | Counter32 | R
.50 | TxFrames6 | Counter32 | R
.51 | TxFrames5 | Counter32 | R
.52 | TxFrames2 | Counter32 | R
.53 | TxFrames1 | Counter32 | R
.54 | IpAddress | IpAddress | R
.55 | RSSI1 | WlanRSSI | R
.56 | RSSI2 | WlanRSSI | R
.57 | RSSI3 | WlanRSSI | R
.82 | RxAirtime | Counter64 | R
.83 | TxAirtime | Counter64 | R
IfIndex
The WLAN radio index.
Address
MAC Address of the Assigned STA. Range: 6 to 6
VSSIndex
The ifindex of the associated Service Set.
State
description not available Enumerations: none (1) associating (2) associated (3) authenticate (4) authenticated (5) delete (8)
Security
The Security Option of the Station. Enumerations: none (1) wep40 (2) wep104 (3) wpa-psk (4) wpa (5) wpa2 (6)
Node
description not available Enumerations: unknown (1) access-point (2) client (3)
MSDUTx
This attribute counts the total number of packets transmitted to this station.
MSDURx
This attribute counts the total number of packets received from this station.
BytesTx
This attribute counts the total number of octets transmitted to this station.
BytesRx
This attribute counts the total number of octets received from this station.
Rate
This attribute reflects the data rate of the latest packet received from this station, in 500 kbps units. Range: 0 to 600
Signal
This attribute shows the received signal strength in dBm. Range: -110 to 0
Noise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established. Range: -110 to 0
ConnectTime
This attribute records the system uptime at the moment the client successfully finished associated.
TimeoutTStamp
Internal time stamp of the most recent STA timeout poll.
TimeoutCount
Internal counter for number of polls sent to the STA without reply.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of data frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of data frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of data frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of data frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of data frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of data frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of data frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of data frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of data frames that were received at 1 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFrames48
This attribute shows the number of data frames that were transmitted at 48 Mbps.
TxFrames36
This attribute shows the number of data frames that were transmitted at 36 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames18
This attribute shows the number of data frames that were transmitted at 18 Mbps.
TxFrames12
This attribute shows the number of data frames that were transmitted at 12 Mbps.
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames9
This attribute shows the number of data frames that were transmitted at 9 Mbps.
TxFrames6
This attribute shows the number of data frames that were transmitted at 6 Mbps.
TxFrames5
This attribute shows the number of data frames that were transmitted at 5.5 Mbps.
TxFrames2
This attribute shows the number of data frames that were transmitted at 2 Mbps.
TxFrames1
This attribute shows the number of data frames that were transmitted at 1 Mbps.
IpAddress
This attribute shows the IP address of the client. it is only available if any IP frames have been received from the client.
RSSI1
This attribute shows the received signal strength at the first receiver in dBm. The value 0 indicates no connection. Range: -110 to 0
RSSI2
This attribute shows the received signal strength at the second receiver in dBm. The value 0 indicates no connection or no second receiver present. Range: -110 to 0
RSSI3
This attribute shows the received signal strength at the third receiver in dBm. The value 0 indicates no connection or no third receiver present. Range: -110 to 0
RxAirtime
Accumulated estimated time in microseconds for all unidirectional frames received from this station.
TxAirtime
Accumulated estimated time in microseconds for all unidirectional frames transmitted to this station.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH