>> MIB - Management Information Base
>> Table: mpsExtensionVoIPTable - (.1.3.6.1.4.1.272.4.53.6.6.1)
Description: This table contains the additional information of the VoIP extension.
mpsExtensionVoIPTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | Location | ENUM | RW
.3 | Network | NetworkIndex | RW
.4 | AdminStatus | ENUM | D
.5 | AdminBinding | DisplayString | RW
.6 | Facilities | BITS | RW
.7 | IpAddressInfo | IpAddress | R
.8 | OperationBinding | DisplayString | R
.9 | OperationStatus | ENUM | R
.10 | CurrentCalls | Counter32 | R
.11 | Codecs | BitValue | RW
.12 | CodecOrder | ENUM | RW
Index
A unique value for additional ip extension settings. Range: 1 to 65535
Location
This value contains the registration location area from which the subscriber is able to setup an VoIP-register. Enumerations: none (1) any (2) nowan (3) lan (4) wan (5) network (6)
Network
If mpsSubsRegistrationLocation = network (6), this value contains the special location index. Range: 1 to 18
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
AdminBinding
This value contains name, port and transport of a static registered client. example: 192.0.0.1:5060;tcp or phone30.bintec.de:5060;upd Data will be used, if mpsExtensionVoIPFacilities static is set. Range: 0 to 64
Facilities
Special facilities of the ip client. static : establish client with fix IP and port, no register possible. g726coding: 0 -> I.366 1 -> RFC 3551/X.420 no-auto-hold: allow multiple connections from this extension. srtp: allow SRTP negotiation Enumerations: static (0) g726coding (1) no-auto-hold (2) srtp (3)
IpAddressInfo
This value contains the ipAdress of the dynamic registered client, to show info in UI.
OperationBinding
This value contains name:port of the registered client, to show info in UI. Range: 0 to 32
OperationStatus
This value contains the actual operation status. notregistered : client is not registered registering : notregistered, registration pending registered : client is registered reregistering : registered, reregistration pending Enumerations: notregistered (1) registering (2) registered (3) reregistering (4)
CurrentCalls
This value contains the current calls.
Codecs
The supported Codecs of the Provider set one or more of the following bit values: ulaw (1) alaw (2) g729 (4) g726 (8) g726_16 (16) g726_32 (32) g726_40 (64) g728 (128) g723_63 (256) g723_53 (512) g729_e (1024) gsm (2048) dtmf (4096) . Default ulaw, alaw and g.729 Range: 0 to -1
CodecOrder
Sorting the codecs default -> system default order quality -> highest quality first lowest -> lowest bandwith first highest -> highest bandwith first Enumerations: default (1) quality (2) lowest (3) highest (4)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH