>> MIB - Management Information Base
>> Table: dot1dStaticDenyTable - (.1.3.6.1.4.1.272.4.8.5.2.1)
Description: Filtering information configured into the bridge by (local or network) management specifying the set of ports to which frames received from a specific port and containing a specific destination address are denied to be forwarded.
dot1dStaticDenyTable
OID | Name | Type | Access
.1 | SrcIfIndex | INTEGER | RW
.2 | DstIfIndex | INTEGER | RW
.3 | ByteOffset | INTEGER | RW
.4 | Mask | OCTET STRING | RW
.5 | Value | OCTET STRING | RW
.6 | Status | ENUM | D
.7 | Age | TimeTicks | RW
SrcIfIndex
Either the value '0', or the port number of the port from which a frame must be received in order for this entry's filtering information to apply. A value of zero indicates that this entry applies on all ports of the bridge for which there is no other applicable entry.
DstIfIndex
Either the value '0', or the port number of the port to which a frame can be forwarded. A value of zero indicates that this entry applies on all ports of the bridge for which there is no other applicable entry.
ByteOffset
Number of bytes in the packet, which are skipped before making the comparison. Range: 0 to 65535
Mask
This octet string specifies which bytes are compared. Leading 0's are handled as when using dot1dStaticDenyByteOffset. Range: 0 to 64
Value
This octet string indicates the value of the bytes to look for. For example: Offset=12 Offset=0 Mask=ff:ff Mask=0:0:0:0:0:0:0:0:0:0:0:0:ff:ff Value=81:37 Value=0:0:0:0:0:0:0:0:0:0:0:0:81:37 Both examples above specify that the 13th byte must be '0x81' and the 14th byte must be '0x37' in order for the filter to match. These examples would deny packets to be bridged. Range: 0 to 64
Status
This object indicates the status of this entry. Enumerations: other (1) invalid (2) permanent (3) deleteOnReset (4) deleteOnTimeout (5)
Age
Age of the entry in seconds.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH