>> MIB - Management Information Base
>> Table: mpsTrunkGroupVoIPTable - (.1.3.6.1.4.1.272.4.53.3.4.1)
Description: This table contains information for each external IP provider.
mpsTrunkGroupVoIPTable
OID | Name | Type | Access
.1 | Index | TrunkGroupIndex | RW
.2 | Type | ENUM | RW
.3 | Mode | ENUM | RW
.4 | Descr | DisplayString | RW
.5 | Bundle | INTEGER | RW
.6 | Domain | DisplayString | RW
.7 | IpAddress | IpAddress | RW
.8 | UserAccount | DisplayString | RW
.9 | AuthName | DisplayString | RW
.10 | AuthPassword | DisplayString | RW
.11 | Facilities | BITS | RW
.12 | Network | NetworkIndex | RW
.13 | InviteTimeout | INTEGER | RW
.14 | AdminStatus | ENUM | D
.15 | OperationStatus | ENUM | R
.16 | TestCommand | ENUM | RW
.17 | TestResult | ENUM | R
.18 | CurrentCalls | Counter32 | R
.19 | ReregisterTimer | INTEGER | RW
.20 | Codecs | BitValue | RW
.21 | CodecOrder | ENUM | RW
.22 | Proxy | DisplayString | RW
.23 | STUNServer | DisplayString | RW
Index
A unique value for each trunk group. Range: 1 to 65535
Type
This value determine the type of the VoIP. Enumerations: sip (1) h323 (2)
Mode
This value determine the mode of the VoIP. Enumerations: pmp (1) pp (2)
Descr
Contains mode of device. Range: 0 to 20
Bundle
This value contains the number of the bundle for this provider.
Domain
This value contains name, port and transport of the registrar. example: 192.0.0.1:5060;tcp or phone30.bintec.de:5060;upd Range: 0 to 64
IpAddress
This value contains ip adress of the registrar.
UserAccount
This value contains the user account. Range: 0 to 64
AuthName
This value contains authorisation name. Range: 0 to 64
AuthPassword
This value contains authorisation password. Range: 0 to 32
Facilities
Special facilities of the IP provider. internationalNumber : Generate international phone number. CLIR : Deactivate number suppression. UseUserID : Use UserID as phone number. notRegistered : Not registered with voip-provider. logInProxy : Allow login of a proxy. compression : voice compression useAreaCode : add area code to dialed number noHoldRetrieve: no hold/retrieve message to the provider replaceIntPrefix: replace intern. prefix (e.g. '00) to '+' clrProvBind: clear provider binding natPing: If set to 0 no NAT ping packets will be send. Set to 1 periodic NAT ping packets will be send. g726coding: 0 -> I.366 1 -> RFC 3551/X.420 earlyConnect: allow early SIP connect srtp: allow SRTP negotiation Enumerations: internationalNumber (0) clir (1) useUserID (2) notRegistered (3) logInProxy (4) compression (5) useAreaCode (6) noHoldRetrieve (7) replaceIntPrefix (8) clrProvBind (9) natPing (10) g726coding (11) earlyConnect (12) srtp (13)
Network
This value contains the special location index. Range: 1 to 18
InviteTimeout
This value contains the size for the end of dial timer.
AdminStatus
Voip Provider is active or not active. Set to delete, to discard teh whole entry. Enumerations: enable (1) disable (2) delete (3)
OperationStatus
This value contains the actual operation status. notregistered : client is not registered registering : notregistered, registration pending registered : client is registered reregistering : registered, reregistration pending Enumerations: notregistered (1) registering (2) registered (3) reregistering (4)
TestCommand
This value contains the current status. Set to test, to test the voip provider. Enumerations: idle (1) test (2)
TestResult
This value contains the current status. Set to test, to test the voip provider. Enumerations: idle (1) progress (2) success (3) error (4)
CurrentCalls
This value contains the current calls.
ReregisterTimer
This value contains reregistering timer in seconds.
Codecs
The supported Codecs of the Provider set one or more of the following bit values: ulaw (1) alaw (2) g729 (4) g726 (8) g726_16 (16) g726_32 (32) g726_40 (64) g728 (128) g723_63 (256) g723_53 (512) g729_e (1024) gsm (2048) dtmf (4096) . Default ulaw, alaw and g.729 Range: 0 to -1
CodecOrder
Sorting the codecs default -> system default order quality -> highest quality first lowest -> lowest bandwith first highest -> highest bandwith first Enumerations: default (1) quality (2) lowest (3) highest (4)
Proxy
This value contains name, port and transport of the outbound proxy. example: 192.0.0.1:5060;tcp or phone30.bintec.de:5060;upd Range: 0 to 64
STUNServer
This value contains name, port and transport of the STUN server. example: 192.0.0.1:5060;tcp or phone30.bintec.de:5060;upd Range: 0 to 64

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH