>> MIB - Management Information Base
>> Table: biboAdmCardTable - (.1.3.6.1.4.1.272.4.1.42.1)
Description: The biboAdmCardTable lists installed cards.
biboAdmCardTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Type | DisplayString | R
.3 | State | ENUM | R
.4 | CpldVersion | DisplayString | R
.5 | FpgaVersion | DisplayString | R
.6 | Temp | INTEGER | R
.7 | TempAlarmThreshold | INTEGER | RW
.8 | TempAlarmTrap | ENUM | R
.9 | Admin | ENUM | RW
Slot
The slot, or location of this card. Range: 0 to 31
Type
The name of this card. Range: 0 to 255
State
State of the card. Enumerations: down (1) running (2) fail (3) stopped (4) stopping (5) starting (6)
CpldVersion
Version of onboard CPLD. Range: 0 to 255
FpgaVersion
Version of loaded FPGA firmware. Range: 0 to 255
Temp
This variable shows the actual card temperature in the unit Celsius. Range: 0 to 250
TempAlarmThreshold
Card temperature threshold. Range: 0 to 250
TempAlarmTrap
If the card temperature raises above the threshold, a trap is generated every 60 seconds. Enumerations: normal (1) critical (2)
Admin
Administrative manipulation of card state. Enumerations: up (1) down (2) reconfig (3)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH