>> MIB - Management Information Base
>> Table: mpsExtensionAdminTable - (.1.3.6.1.4.1.272.4.53.6.2.1)
Description: This table contains extended settings for internal extension.
mpsExtensionAdminTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | DialAuthorisation | ENUM | RW
.3 | Facilities | BITS | RW
.4 | PickupGroup | INTEGER | RW
.5 | PhonebookAccess | ENUM | RW
.6 | MusicOnHold | ENUM | RW
.7 | AdminStatus | ENUM | D
Index
A unique value for each extensions. Range: 1 to 65535
DialAuthorisation
Dialing privileges for a extension specifies what type of calls (internal, external, etc. ) this extension can place. Default is international. Enumerations: unknown (1) international (2) incoming (3) national (4) region (5) internal (6) onlyDoorIntercom (7) local (8)
Facilities
Special facilities of the extension. suppress-A-Addr : Suppress outgoing CLIP information (CLIR). suppress-B-Addr : This value determine if Suppress number of called party (COLR) is enabled or not. store-charge : Charge information for this subscriber will be record or not. doorIntercom-access : Authorizes an internal subscriber to establish a connection with the door entry phone or open the door. auto-trunk-req : This setting defines whether automatic access to an outside line is to be configured for the selected subscriber. keypad : Authorizes an internal subscriber to carry out keypad functions. route-barring: If you have configured the dialing filter (consisting of an inhibit and release filter) in the PABX system you can use these settings to define whether the selected subscriber is subject to the constraints/privileges imposed/offered by the dialing filter. add-trunk-acc-dig : The line access code is placed in front of the number automatically by the PABX system for incoming external calls. rma-access : This permits a subscriber to activate the service access to the PABX system, or to establish a corresponding service connection on their own. extern-diversion : You can use this setting to define whether external call forwarding for the internal subscriber is to be executed within the PABX system or at the exchange. extern-hold : You can use this setting to define whether external call hold for the internal subscriber is to be executed within the PABX system or at the exchange. add-line-acc-dig : The internal dialing code is places in front of the number automatically by the PABX system for incoming internal calls. msg-waiting : Message waiting indication on or off time-lock : If on, the access rights will be changed at a time specified in the calendar. sms : Authorizes an internal subscriber to receive SMS messages. rma-user-access : Authorization for remote access activation is on or off. tapi : Authorizes a subscriber to use the PABX's TAPI features. ccnr : The completion of call on no answer (CCNR) feature is available to the user. . Enumerations: suppress-A-Addr (0) suppress-B-Addr (1) store-charge (2) doorIntercom-access (3) auto-trunk-req (4) keypad (5) route-barring (6) add-trunk-acc-dig (7) rma-access (8) extern-diversion (9) extern-hold (10) add-line-acc-dig (11) msg-waiting (12) time-lock (13) sms (14) rma-user-access (15) tapi (16) ccnr (17)
PickupGroup
Enter the number of the group in which calls are to be taken.
PhonebookAccess
This value determine the access to the pbx phonebook. Enumerations: denied (1) restricted (2) unrestricted (3)
MusicOnHold
This value contains the selected music on hold (MoH) that a party is to hear that has been transferred by the selected internal subscriber. Enumerations: file1 (1) file2 (2) file3 (3) file4 (4) file5 (5) file6 (6) file7 (7) file8 (8) dialtone (50) default1 (51) default2 (52) external (80)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH