>> MIB - Management Information Base
>> Table: userAlert - (.1.3.6.1.4.1.272.4.43.2)
userAlert
OID | Name | Type | Access
.1 | AdminStatus | ENUM | RW
.2 | SMTPHost | DisplayString | RW
.3 | Origin | DisplayString | RW
.4 | Mails | INTEGER | RW
.5 | Error | DisplayString | R
.6 | Authentication | ENUM | RW
.7 | POP3Host | DisplayString | RW
.8 | POP3valid | INTEGER | RW
.9 | User | DisplayString | RW
.10 | Pass | DisplayString | RW
AdminStatus
Disable or enable user Alert Enumerations: enable (1) disable (2)
SMTPHost
SMTP Server for outgoing emails Range: 0 to 60
Origin
SMTP originator Range: 0 to 60
Mails
Maximum Mails per minute Range: 1 to 30
Error
Display last SMTP error Range: 0 to 60
Authentication
SMTP Server Authentication mode Enumerations: none (1) esmtp (2) pop3 (3)
POP3Host
POP3 Server for SMTP after POP Range: 0 to 60
POP3valid
POP3 login valid for xx seconds Range: 30 to 3600
User
Username for SMTP Login Range: 0 to 40
Pass
Password for SMTP Login Range: 0 to 40

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH