>> MIB - Management Information Base
>> Table: ospfVirtIfTable - (.1.3.6.1.2.1.14.9.1)
Description: Information about a single Virtual Interface.
ospfVirtIfTable
OID | Name | Type | Access
.1 | AreaId | IpAddress | RW
.2 | Neighbor | IpAddress | RW
.3 | TransitDelay | INTEGER | RW
.4 | RetransInterval | INTEGER | RW
.5 | HelloInterval | INTEGER | RW
.6 | RtrDeadInterval | INTEGER | RW
.7 | State | ENUM | R
.8 | Events | Counter | R
.9 | AuthKey | DisplayString | RW
.10 | Status | ENUM | D
.11 | AuthType | INTEGER | RW
AreaId
The Transit Area that the Virtual Link traverses. By definition, this is not 0.0.0.0
Neighbor
The Router ID of the Virtual Neighbor.
TransitDelay
The estimated number of seconds it takes to transmit a link- state update packet over this interface. Range: 1 to 3600
RetransInterval
The number of seconds between link-state ad- vertisement retransmissions, for adjacencies belonging to this interface. This value is also used when retransmitting database descrip- tion and link-state request packets. This value should be well over the expected round- trip time. Range: 1 to 3600
HelloInterval
The length of time, in seconds, between the Hello packets that the router sends on the in- terface. This value must be the same for the virtual neighbor. Range: 1 to 65535
RtrDeadInterval
The number of seconds that a router's Hello packets have not been seen before it's neigh- bors declare the router down. This should be some multiple of the Hello interval. This value must be the same for the virtual neigh- bor.
State
OSPF virtual interface states. Enumerations: down (1) pointToPoint (4)
Events
The number of state changes or error events on this Virtual Link
AuthKey
If Authentication Type is simplePassword, the device will left adjust and zero fill to 8 oc- tets. Note that unauthenticated interfaces need no authentication key, and simple password authen- tication cannot use a key of more than 8 oc- tets. Larger keys are useful only with authen- tication mechanisms not specified in this docu- ment. When read, ospfVirtIfAuthKey always returns a string of length zero. Range: 0 to 255
Status
This variable displays the status of the en- try. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)
AuthType
The authentication type specified for a virtu- al interface. Additional authentication types may be assigned locally. Range: 0 to 255

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH