>> MIB - Management Information Base
>> Table: ipSifAliasServiceTable - (.1.3.6.1.4.1.272.4.5.29.1)
Description: Contains a alias Service Entry Protocol,Port,Range
ipSifAliasServiceTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Alias | DisplayString | RW
.3 | Protocol | ENUM | D
.4 | Port | INTEGER | RW
.5 | Range | INTEGER | RW
.6 | Type | ENUM | R
.7 | Group | INTEGER | RW
.8 | SourcePort | INTEGER | RW
.9 | SourceRange | INTEGER | RW
.10 | IcmpType | INTEGER | RW
.11 | IcmpCode | INTEGER | RW
Index
The Index for the address alias
Alias
Alias Name for the Service Entry Range: 0 to 255
Protocol
The protocol for the Service alias Enumerations: icmp (1) igmp (2) ggp (3) ip (4) tcp (6) egp (8) igp (9) pup (12) chaos (16) udp (17) hmp (20) xns-idp (22) rdp (27) ipv6 (41) rsvp (46) gre (47) esp (50) ah (51) tlsp (56) skip (57) kryptolan (65) iso-ip (80) igrp (88) ospf (89) ipip (94) pim (103) ipx-in-ip (111) vrrp (112) l2tp (115) local (250) internet (251) netmeeting (252) udptcp (253) any (254) delete (255) dont-verify (256)
Port
The Port for the Service Alias. Range: -1 to 65535
Range
The Port Range for the Service Alias. Range: 1 to 65536
Type
Specifies wether created by the IP/SIF subsystem itself or created/modified by the administrator. Enumerations: predefined (1) custom (2)
Group
For values greater than zero this entry determines the IP service group this entry belongs to, see also ipSifAliasServiceGroupId Range: 0 to 100
SourcePort
The Source Port for the Service Alias. Range: 0 to 65535
SourceRange
The Source Port Range for the Service Alias. Range: 1 to 65536
IcmpType
The ICMP Type for the Service Alias. Range: -1 to 255
IcmpCode
The ICMP Code for the Service Alias. Range: -1 to 255

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH