>> MIB - Management Information Base
>> Table: capiNcciTable - (.1.3.6.1.4.1.272.4.7.4.1)
Description: The capiNcciTable contains information for each CAPI NCCI (network control connection identifier). An NCCI describes a logical connection on level 3. Several NCCIs operating on the same PLCI may exist. Creating entries: As soon as a CAPI_CONNECT_B3_REQ (or CAPI_CONNECT_B3_IND) message is received, the system creates an entry by assigning the application a unique capiNcciNumber. Deleting entries: Entries are automatically deleted by the system once a CAPI_DISCONNECT_B3_RESP message is received.
capiNcciTable
OID | Name | Type | Access
.1 | Number | HexValue | R
.2 | Application | INTEGER | R
.3 | Plci | HexValue | R
.4 | State | ENUM | R
Number
The NCCI number assigned by the system. Range: 0 to -1
Application
The application number (capiApplNumber).
Plci
The CAPI PLCI number (capiPlciNumber). Range: 0 to -1
State
The current state of the NCCI, as described in the CAPI state diagram. Enumerations: n-0 (1) n-1 (2) n-2 (3) n-3 (4) n-4 (5) n-5 (6) n-act (7)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH