>> MIB - Management Information Base
>> Table: voipExtensionTable - (.1.3.6.1.4.1.272.4.33.2.1)
Description: Settings of an extension entry common to all extension types.
voipExtensionTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Number | DisplayString | RW
.3 | Alias | DisplayString | RW
.4 | Mask | BitValue | RW
.5 | Type | ENUM | D
.9 | OperStatus | ENUM | R
Index
Unique index of this extension entry. Range: 1 to 65535
Number
Assigned number or prefix for this extension. Range: 0 to 32
Alias
An internal alias assigned to this extension. This parameter is currently unused. Range: 0 to 32
Mask
Interface stack mask position of a referenced interface (ISDN stack or MGCP UNITS). This entry can only be set for 'voipExtensionType' = 'analog' and 'digital' (and theoretically 'mgcp'). For all other types this variable is empty. For 'analog' and 'digital' interfaces the needed value can be found in the interface's isdnStkTable entry at 'isdnstkNumber' (= the bitmask position of the interface in the stack's bitmask). Note that despite the BitValue data type of this parameter no bitmask is entered here, just the 'isdnstkNumber' integer value of a single interface. Range: 0 to -1
Type
Interface type of extension. 'analog' (POTS), 'digital' (ISDN), SIP, MGCP, H.323 (or 'delete'). MGCP and H.323 are currently not implemented. Enumerations: analog (1) digital (2) sip (3) h323 (4) mgcp (5) delete (7)
OperStatus
Current operational state of connected extension. Enumerations: down (11) dormant (12) trying (13) register (14) authenticate (15) up (16) failed (17) blocked (18) disable (19)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH