>> MIB - Management Information Base
>> Table: mpsDeviceTable - (.1.3.6.1.4.1.272.4.53.3.1.1)
Description: This table contains information of each physical device (internal and external).
mpsDeviceTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RW
.2 | Mode | ENUM | RW
.3 | DisplayName | DisplayString | RW
.4 | Bundle | INTEGER | RW
.5 | TrunkGroup | TrunkGroupIndexOrZero | RW
.6 | DefaultExtension | ExtensionIndexOrZero | RW
.7 | BusMode | ENUM | RW
.8 | ClipNoScreening | ENUM | RW
.9 | AdminStatus | ENUM | D
IfIndex
A unique value for each device. Range: 1 to 2147483647
Mode
Contains mode of the device. Enumerations: none (1) itrunk-pmp (2) itrunk-pp (3) iline-pmp (4) iline-pp (5) analine (6) itrunk-pp-S2m (7) dectline (8) anatrunk (9)
DisplayName
Display name of the device. Range: 0 to 32
Bundle
This value contains the bundle number of the device.
TrunkGroup
A unique value for each trunk group index. Range: 0 to 65535
DefaultExtension
Contains the extension index of an internal device port, for default. Range: 0 to 65535
BusMode
The configuration of the internal isdn device port is standard(1) or extended(2) Enumerations: standard (1) extended (2)
ClipNoScreening
This value determine when the mpsDeviceMode = itrunk-pp, wether ClipNoScreening is disabled(1) or individual(2) or global(3). Enumerations: no (1) individual (2) global (3)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2) disable (3)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH