>> MIB - Management Information Base
>> Table: mpsSysConfig - (.1.3.6.1.4.1.272.4.53.1.1)
mpsSysConfig
OID | Name | Type | Access
.1 | Country | ENUM | RW
.2 | SetExchangeDate | ENUM | RW
.3 | Facilities | BITS | RW
.4 | AreaCode | DisplayString | RW
.5 | CountryCode | DisplayString | RW
.6 | CodeInternationalPrefix | DisplayString | RW
.7 | CodeNationalPrefix | DisplayString | RW
Country
This value contains the country code settings. Enumerations: germany (1) netherlands (2) united-kindom (3) belgium (4) italy (5) denmark (6) spain (7) sweden (8) norway (9) france (10) portugal (11) austria (12) switzerland (13) czech (14) slovenia (15) poland (16) hungary (17) greece (18)
SetExchangeDate
Accept time and date is off, acceppt from exchange or accept from time server. Enumerations: no (1) pbx (2) time-server (3)
Facilities
System facilities. highRingerFrequency : a/b extension ringing frequency handoverBusyExtension : This value determine if handover to busy extension is possible handoverBusyMusicOnHold : This value determine if the caller hear tone or moh Enumerations: highRingerFrequency (0) handoverBusyExtension (1) handoverBusyMusicOnHold (2)
AreaCode
This value contain the digit for the national prenum. Range: 0 to 10
CountryCode
This value contain the digit for the international prenum. Range: 0 to 6
CodeInternationalPrefix
This value contain the digits for international prefix code. Range: 0 to 2
CodeNationalPrefix
This value contain the digits for national prefix code. Range: 0 to 1

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH