>> MIB - Management Information Base
>> Table: ipNetToMediaTable - (.1.3.6.1.2.1.4.22.1)
Description: Each entry contains one IpAddress to `physical' address equivalence.
ipNetToMediaTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RC
.2 | PhysAddress | PhysAddress | RC
.3 | NetAddress | IpAddress | RC
.4 | Type | ENUM | D
IfIndex
The interface on which this entry's equivalence is effective. The interface identified by a particular value of this index is the same interface as identified by the same value of RFC 1573's ifIndex. Range: 1 to 2147483647
PhysAddress
The media-dependent `physical' address.
NetAddress
The IpAddress corresponding to the media-dependent `physical' address.
Type
The type of mapping. Setting this object to the value invalid(2) has the effect of invalidating the corresponding entry in the ipNetToMediaTable. That is, it effectively disassociates the interface identified with said entry from the mapping identified with said entry. It is an implementation- specific matter as to whether the agent removes an invalidated entry from the table. Accordingly, management stations must be prepared to receive tabular information from agents that corresponds to entries not currently in use. Proper interpretation of such entries requires examination of the relevant ipNetToMediaType object. Enumerations: other (1) invalid (2) dynamic (3) static (4)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH