>> MIB - Management Information Base
>> Table: hdsl2ShdslEndpointConfTable - (.1.3.6.1.4.1.272.4.35.1.1.4.1)
Description: An entry in the hdsl2ShdslEndpointConfTable. Each entry represents a single segment endpoint in a HDSL2/SHDSL line. It is indexed by the ifIndex of the HDSL2/SHDSL line, the UnitId of the associated unit, the side of the unit, and the wire-pair of the associated modem.
hdsl2ShdslEndpointConfTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Side | ENUM | RW
.5 | WireInterface | ENUM | RW
.6 | MinLineRate | INTEGER | RW
.7 | MaxLineRate | INTEGER | RW
.8 | TransmissionMode | ENUM | RW
.11 | WorstCaseTargetMarginDown | INTEGER | RW
.13 | WorstCaseTargetMarginUp | INTEGER | RW
.14 | GroupId | INTEGER | RW
.15 | LineProbeEnable | ENUM | RW
.16 | LicenseUsage | ENUM | R
IfIndex
This object specifies the associated interface index of this HDSL2/SHDSL line.
Side
The side of the unit associated with this segment endpoint - Network/Customer side - as per the Hdsl2ShdslUnitSide textual convention. Enumerations: networkSide (1) customerSide (2)
WireInterface
This object configures the two-wire or optional four-wire operation for this SHDSL segment. Enumerations: twoWire (1) fourWire (2) fourWireStandard (3) fourWireIMA (4) sixWire (5) sixWireIMA (6) eightWire (7) eightWireIMA (8) not-used (9) groupMember (10)
MinLineRate
This object configures the minimum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
MaxLineRate
This object configures the maximum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
TransmissionMode
This object specifies the regional setting for the SHDSL line: region1 - ITU-T G.991.2 Annex A region2 - ITU-T G.991.2 Annex B Enumerations: region1 (1) region2 (2) region1or2 (3)
WorstCaseTargetMarginDown
This object specifies the downstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: 0 to 65535
WorstCaseTargetMarginUp
This object specifies the upstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 21
GroupId
This object defines which wire-pairs belong to the same M-pair group or IMA group. Members of the same group have the same entry. Range: 0 to 255
LineProbeEnable
This object specifies the configuration of the PMMS behavior: auto - Line Probe is enabled if hdsl2ShdslEndpointConfMinLineRate < hdsl2ShdslEndpointConfMaxLineRate. disable - Line Probe is disabled. enable - Line Probe is enabled. Enumerations: auto (1) disable (2) enable (3)
LicenseUsage
Shows which license type is currently used for this SHDSL interface. Enumerations: none (1) missing (2) shdsl (3)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH