>> MIB - Management Information Base
>> Table: mpsExtensionDiversionTable - (.1.3.6.1.4.1.272.4.53.6.9.1)
Description: This table contains the configured diversions.
mpsExtensionDiversionTable
OID | Name | Type | Access
.1 | Index | ExtensionIndex | RW
.2 | Service | ENUM | RW
.3 | CFU | DisplayString | RW
.4 | CFB | DisplayString | RW
.5 | CFNR | DisplayString | RW
.6 | CFU2 | DisplayString | RW
.7 | CFU3 | DisplayString | RW
.8 | CFU3Fixed | ENUM | RW
.9 | CFU3Active | ENUM | RW
.10 | AdminStatus | ENUM | D
Index
A unique value for the extension, who has configured this diversion. Range: 1 to 65535
Service
Diversion for a special service. Enumerations: no (1) telephone (2) telephone3k1hz (3) telephoneAnalog (4) telephone7k1hz (5) analog (6) analogFaxG2 (7) analogFaxG3 (8) dataViaModem (9) btxViaModem (10) x21 (11) x21Uc4 (12) x21Uc5 (13) x21Uc6 (14) x21Uc19 (15) telefaxG4 (16) btx64kbit (17) data64kbit (18) x25 (19) x25Uc8 (20) x25Uc9 (21) x25Uc10 (22) x25Uc11 (23) x25Uc13 (24) x2519k2hz (25) teletex64 (26) mixedMode (27) telematicControl (28) grafiktelefondienste (29) btxNew (30) videoTelephone (31) videoTelephone3k1hz (32) videoTelephone7khz (33) videoTelephonePicture (34) speech (35) unrestrictedDigitalInformation (36) audio3k1 (37) audio7k (38) videotextInternational (39) allServices (40)
CFU
Destination number. Range: 0 to 24
CFB
Destination number. Range: 0 to 24
CFNR
Destination number. Range: 0 to 24
CFU2
This value contains the diversion target number for call deflection. Range: 0 to 24
CFU3
This value contains the diversion target number for follow me. Range: 0 to 24
CFU3Fixed
This value determine whether the follow me diversion (CFU3) is fixed(1) or variable(2). Enumerations: true (1) false (2)
CFU3Active
This value determine whether the follow me diversion (CFU3) is active(1) or not active(2). Enumerations: true (1) false (2)
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH