>> MIB - Management Information Base
>> Table: mpsDoorIntercomModeTable - (.1.3.6.1.4.1.272.4.53.7.4.1)
Description: This table contains the information of each doorline and variant.
mpsDoorIntercomModeTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | Button | DoorButtonIndex | RW
.3 | Number | GroupModeIndex | RW
.4 | Handling | ENUM | RW
.5 | Assignment | ENUM | RW
.6 | ExtNumber | DisplayString | RW
.7 | AdminStatus | ENUM | D
Index
A unique value for each door intercom. Range: 1 to 10
Button
A unique value for each door intercom. Range: 1 to 4
Number
For each door intercom a variant. Range: 1 to 2
Handling
Signalling mode (internal) of the door intercom group. Enumerations: simultaneous (1) linear (2) rotating (3) adding (4) linear-ext (5) rotating-ext (6)
Assignment
Door intercom group member are internal or external Enumerations: internal (1) external (2)
ExtNumber
This external number will be called, if mpsDoorIntercomModeAssignment = external. Range: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH