>> MIB - Management Information Base
>> Table: voipCallHistoryTable - (.1.3.6.1.4.1.272.4.33.4.1)
Description: Defintion of a VoIP call history entry. Only finished calls are stored here. (counterpart to the the isdnCallHistoryTable).
voipCallHistoryTable
OID | Name | Type | Access
.1 | TimeStamp | Date | R
.2 | Duration | TimeTicks | R
.3 | ProtocolType | ENUM | R
.4 | DisconnectCause | DisplayString | R
.5 | Role | ENUM | D
.6 | RefValue | INTEGER | R
.7 | Id | OCTET STRING | R
.8 | LocalNumber | DisplayString | R
.9 | LocalAlias | DisplayString | R
.10 | LocalIpAddr | IpAddress | R
.11 | LocalIpPort | INTEGER | R
.12 | RemoteNumber | DisplayString | R
.13 | RemoteAlias | DisplayString | R
.14 | RemoteIpAddr | IpAddress | R
.15 | RemoteIpPort | INTEGER | R
.16 | RemoteEndpointVendor | DisplayString | R
.17 | NegotiatedCodec | ENUM | R
.18 | TxPacketLengthMs | INTEGER | R
.19 | TxPackets | Counter32 | R
.20 | TxOctets | Counter32 | R
.21 | RxPacketLengthMs | INTEGER | R
.22 | RxPackets | Counter32 | R
.23 | RxOctets | Counter32 | R
.24 | If | INTEGER | R
TimeStamp
Timestamp of call (connection) establishment. Range: 0 to -1
Duration
Call duration in hundredth seconds.
ProtocolType
VoIP protocol used during call. Enumerations: h323 (1) mgcp (2) sip (3) ipi (4)
DisconnectCause
Saves disconnect reason of the call. Range: 0 to 255
Role
Endpoint's role within finished call. Enumerations: caller (1) called (2) delete (3)
RefValue
Unique number which identifies call (conforming to Q.931). Range: 0 to 32767
Id
Call-ID of associated call.
LocalNumber
Internal number of local user. Range: 0 to 255
LocalAlias
Optional alias of local user. Range: 0 to 255
LocalIpAddr
IP address used by local user.
LocalIpPort
Associated port number used by local user. Range: 1 to 65535
RemoteNumber
Number of remote user if available. Range: 0 to 255
RemoteAlias
Alias of remote user if available. Range: 0 to 255
RemoteIpAddr
IP address used by remote user.
RemoteIpPort
Associated port number used by remote user. Range: 1 to 65535
RemoteEndpointVendor
Vendor's product description used by remote user. Range: 0 to 255
NegotiatedCodec
Codec negotiated during connection establishment. Enumerations: g711a (1) g711u (2) g723-53 (3) g723-63 (4) g726-16 (5) g726-24 (6) g726-32 (7) g726-40 (8) g728 (9) g729 (10) g729a (11) g729b (12) t38udp (13) t38tcp (14) gsm (15) g722 (16) data (17) dtmf (18)
TxPacketLengthMs
Audio data length in milliseconds transmitted in a single frame. Range: 1 to 255
TxPackets
Number of RTP packets transmitted.
TxOctets
Number of octets transmitted.
RxPacketLengthMs
Audio data length in milliseconds received in a single frame. Range: 1 to 255
RxPackets
Number of RTP packets received.
RxOctets
Number of octets received.
If
Call-ID of associated call.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH