>> MIB - Management Information Base
>> Table: dot11SupportedDataRatesRxTable - (.1.2.840.10036.4.10.1)
Description: An Entry (conceptual row) in the dot11SupportedDataRatesRx Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11SupportedDataRatesRxTable
OID | Name | Type | Access
.1 | Index | Integer32 | R
.2 | Value | Integer32 | R
Index
Index object which identifies which data rate to access. Range is 1..255. Range: 1 to 255
Value
The receive bit rates supported by the PLCP and PMD, represented by a count from X'02-X'7f, corresponding to data rates in increments of 500Kb/s from 1 Mb/s to 63.5 Mb/s. Range: 2 to 127

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH