>> MIB - Management Information Base
>> Table: wlanWDSHTStatsTable - (.1.3.6.1.4.1.272.4.46.18.1)
Description: The wlanWDSHTStatsTable contains additional statistical data about 802.11n HT frames for WDS links. Each entry corresponds to an wlanWDSTable entry. Entries cannot be added or deleted by the user.
wlanWDSHTStatsTable
OID | Name | Type | Access
.1 | RxFramesMCS0 | Counter32 | R
.2 | RxFramesMCS1 | Counter32 | R
.3 | RxFramesMCS2 | Counter32 | R
.4 | RxFramesMCS3 | Counter32 | R
.5 | RxFramesMCS4 | Counter32 | R
.6 | RxFramesMCS5 | Counter32 | R
.7 | RxFramesMCS6 | Counter32 | R
.8 | RxFramesMCS7 | Counter32 | R
.9 | RxFramesMCS8 | Counter32 | R
.10 | RxFramesMCS9 | Counter32 | R
.11 | RxFramesMCS10 | Counter32 | R
.12 | RxFramesMCS11 | Counter32 | R
.13 | RxFramesMCS12 | Counter32 | R
.14 | RxFramesMCS13 | Counter32 | R
.15 | RxFramesMCS14 | Counter32 | R
.16 | RxFramesMCS15 | Counter32 | R
.17 | TxFramesMCS0 | Counter32 | R
.18 | TxFramesMCS1 | Counter32 | R
.19 | TxFramesMCS2 | Counter32 | R
.20 | TxFramesMCS3 | Counter32 | R
.21 | TxFramesMCS4 | Counter32 | R
.22 | TxFramesMCS5 | Counter32 | R
.23 | TxFramesMCS6 | Counter32 | R
.24 | TxFramesMCS7 | Counter32 | R
.25 | TxFramesMCS8 | Counter32 | R
.26 | TxFramesMCS9 | Counter32 | R
.27 | TxFramesMCS10 | Counter32 | R
.28 | TxFramesMCS11 | Counter32 | R
.29 | TxFramesMCS12 | Counter32 | R
.30 | TxFramesMCS13 | Counter32 | R
.31 | TxFramesMCS14 | Counter32 | R
.32 | TxFramesMCS15 | Counter32 | R
.33 | RxBandwidth | ENUM | R
.34 | RxGuardInterval | ENUM | R
.35 | TxBandwidth | ENUM | R
.36 | TxGuardInterval | ENUM | R
RxFramesMCS0
This attribute shows the number of HT data frames that were received at MCS 0.
RxFramesMCS1
This attribute shows the number of HT data frames that were received at MCS 1.
RxFramesMCS2
This attribute shows the number of HT data frames that were received at MCS 2.
RxFramesMCS3
This attribute shows the number of HT data frames that were received at MCS 3.
RxFramesMCS4
This attribute shows the number of HT data frames that were received at MCS 4.
RxFramesMCS5
This attribute shows the number of HT data frames that were received at MCS 5.
RxFramesMCS6
This attribute shows the number of HT data frames that were received at MCS 6.
RxFramesMCS7
This attribute shows the number of HT data frames that were received at MCS 7.
RxFramesMCS8
This attribute shows the number of data frames that were received at MCS 8.
RxFramesMCS9
This attribute shows the number of HT data frames that were received at MCS 9.
RxFramesMCS10
This attribute shows the number of HT data frames that were received at MCS 10.
RxFramesMCS11
This attribute shows the number of HT data frames that were received at MCS 11.
RxFramesMCS12
This attribute shows the number of HT data frames that were received at MCS 12.
RxFramesMCS13
This attribute shows the number of HT data frames that were received at MCS 13.
RxFramesMCS14
This attribute shows the number of HT data frames that were received at MCS 14.
RxFramesMCS15
This attribute shows the number of HT data frames that were received at MCS 15.
TxFramesMCS0
This attribute shows the number of HT data frames that were transmitted at MCS 0.
TxFramesMCS1
This attribute shows the number of HT data frames that were transmitted at MCS 1.
TxFramesMCS2
This attribute shows the number of HT data frames that were transmitted at MCS 2.
TxFramesMCS3
This attribute shows the number of HT data frames that were transmitted at MCS 3.
TxFramesMCS4
This attribute shows the number of HT data frames that were transmitted at MCS 4.
TxFramesMCS5
This attribute shows the number of HT data frames that were transmitted at MCS 5.
TxFramesMCS6
This attribute shows the number of HT data frames that were transmitted at MCS 6.
TxFramesMCS7
This attribute shows the number of HT data frames that were transmitted at MCS 7.
TxFramesMCS8
This attribute shows the number of data frames that were transmitted at MCS 8.
TxFramesMCS9
This attribute shows the number of HT data frames that were transmitted at MCS 9.
TxFramesMCS10
This attribute shows the number of HT data frames that were transmitted at MCS 10.
TxFramesMCS11
This attribute shows the number of HT data frames that were transmitted at MCS 11.
TxFramesMCS12
This attribute shows the number of HT data frames that were transmitted at MCS 12.
TxFramesMCS13
This attribute shows the number of HT data frames that were transmitted at MCS 13.
TxFramesMCS14
This attribute shows the number of HT data frames that were transmitted at MCS 14.
TxFramesMCS15
This attribute shows the number of HT data frames that were transmitted at MCS 15.
RxBandwidth
This attribute shows the bandwidth the remote side used with the last received frame: 20 MHz (1) or 40 MHz (2). Enumerations: b20MHz (1) b40MHz (2)
RxGuardInterval
This attribute shows the length of the guard interval the remote side used with the last received frame: long (1) or short (2). Enumerations: long (1) short (2)
TxBandwidth
This attribute shows the bandwidth the local side used for transmitting the last frame: 20 MHz (1) or 40 MHz (2). Enumerations: b20MHz (1) b40MHz (2)
TxGuardInterval
This attribute shows the length of the guard interval the local side used for transmitting the last frame: long (1) or short (2). Enumerations: long (1) short (2)

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH