>> MIB - Management Information Base
>> Table: mediaConnTable - (.1.3.6.1.4.1.272.4.50.1.1)
Description: Lists RTP session parameters for monitoring usage.
mediaConnTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | IntAddr | IpAddress | R
.3 | IntPort | INTEGER | R
.4 | ExtAddr | IpAddress | R
.5 | ExtPort | INTEGER | R
.6 | RemoteAddr | IpAddress | R
.7 | RemotePort | INTEGER | R
.8 | Age | TimeTicks | R
Index
Unique ID of entry.
IntAddr
Internal address of RTP stream.
IntPort
Internal port of RTP stream.
ExtAddr
External (public) address of RTP stream.
ExtPort
External (public) port of RTP stream.
RemoteAddr
Destination address of RTP stream.
RemotePort
Destination port of RTP stream.
Age
Age of RTP session.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH