>> MIB - Management Information Base
>> Table: atmIfTable - (.1.3.6.1.4.1.272.4.16.10.1)
Description: An interface entry containing objects at the subnetwork layer and below for a particular interface.
atmIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Type | ENUM | R
.3 | Descr | DisplayString | R
.4 | AdminStatus | ENUM | RW
.5 | OperStatus | ENUM | R
.6 | LastChange | TimeTicks | R
.7 | MaxTxRate | INTEGER | RW
.22 | InPkts | INTEGER | R
.23 | OutPkts | INTEGER | R
.24 | RxSpeed | INTEGER | R
.25 | TxSpeed | INTEGER | R
.26 | InOctets | Counter | R
.27 | InDiscards | Counter | R
.28 | InErrors | Counter | R
.29 | OutOctets | Counter | R
.30 | OutDiscards | Counter | R
.31 | OutErrors | Counter | R
Index
The interface index of the associated ATM hardware.
Type
This object contains an interface type. Enumerations: other (1) adsl (2) shdsl (3)
Descr
Short description for this object. Range: 0 to 255
AdminStatus
This object contains the desired state of the ATM interface. Enumerations: up (1) down (2)
OperStatus
The current operational state of the ATM interface. Enumerations: up (1) down (2)
LastChange
The value of sysUpTime at the time the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this object contains a zero value.
MaxTxRate
This object enables traffic shaping on the related ATM interface. If set to zero (0) there is no shaping active. Otherwise this variable defines the maximum amount of bits per second to be transmitted. Note that the maximum transmit rate is also determined by the capabilities of the ATM hardware.
InPkts
The number of reassembled received packets.
OutPkts
This number of transmitted packets.
RxSpeed
This object contains the receive interface speed.
TxSpeed
This object contains the transmit interface speed.
InOctets
The total number of octets received on the interface, including framing characters.
InDiscards
The number of inbound packets which were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol. One possible reason for discarding such a packet could be to free up buffer space.
InErrors
The number of inbound packets that contained errors preventing them from being deliverable to a higher-layer protocol.
OutOctets
The total number of octets transmitted out of the interface, including framing characters.
OutDiscards
The number of outbound packets which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a packet could be to free up buffer space.
OutErrors
The number of outbound packets that could not be transmitted because of errors.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH