>> MIB - Management Information Base
>> Table: ipHostAccessTable - (.1.3.6.1.4.1.272.4.5.62.1.1)
Description: An entry (conceptual row) representing an interface on which host access authentication is enabled.
ipHostAccessTable
OID | Name | Type | Access
.1 | Status | ENUM | D
.2 | IfIndex | INTEGER | RC
.3 | DefaultPassword | DisplayString | RC
.4 | WalledNetwork | IpAddress | RC
.5 | WalledNetmask | IpAddress | RC
.6 | WalledURL | DisplayString | RC
.7 | TermsURL | DisplayString | RC
.8 | UserDomain | DisplayString | RC
.9 | ReAuthenticatePeriod | Unsigned32 | RC
.10 | DefaultSessionTimeout | Unsigned32 | RC
.11 | DefaultMaxTransfer | Counter64 | RC
.12 | DefaultIdleTimeout | Unsigned32 | RC
.13 | DefaultAcctInterval | Unsigned32 | RC
.14 | SessionTimeReporting | ENUM | RC
.15 | WalledStatus | ENUM | RC
.16 | DefaultLanguage | DisplayString | RC
Status
The status of this entry. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)
IfIndex
The corresponding interface for which host access authentication should be applied.
DefaultPassword
The default password used for authentication. If defined, only a valid vouchure ID is needed for authentication. Range: 0 to 255
WalledNetwork
This object specifies together with ipHostAccessWalledNetmask the network where hosts can communicate without authorization. It can be deactivated via field WalledStatus.
WalledNetmask
The netmask which corresponds to ipHostAccessWalledNetwork. It can be deactivated via field WalledStatus.
WalledURL
The URL of the Walled Garden page shown beside the login-page, e.g. 'http://www.funkwerk-ec.com/'. This page can be deactivated via empty string and/or via field WalledStatus. Range: 0 to 255
TermsURL
The URL of the Terms & Conditions link shown in the login-page, e.g. 'http://www.funkwerk-ec.com/'. This link can be deactivated via empty string and/or via field WalledStatus. Range: 0 to 255
UserDomain
The domain name which automatically will be appended to the username during authentication. Range: 0 to 255
ReAuthenticatePeriod
The re-authentication-period in seconds. A value of 0 is interpreted as NO re-authentications.
DefaultSessionTimeout
The default session-timeout-period in seconds that is used if the Radius-server does not specify it. In deviation from RFC 2865, section 5.27, a value of 0 is interpreted as NO session-timeout.
DefaultMaxTransfer
The default maximum number of received plus sent bytes if the Radius-server does not specify it. 0 means NO limit. Radius standard does not specify any attribute for this maximum.
DefaultIdleTimeout
The default idle-timeout-period in seconds that is used if the Radius-server does not specify it. In deviation from RFC 2865, section 5.28, a value of 0 is interpreted as NO idle-timeout.
DefaultAcctInterval
The default accounting-interim-interval in seconds that is used if the Radius-server does not specify it. In deviation from RFC 2869, section 5.16, a value of 0 means NO interim-updates.
SessionTimeReporting
Toggles calculation of session-time (RFC 2866, section 5.7). For with-idle-time(1), the session-start is subtracted from the current time. For without-idle-time(2), it is subtracted from time of the latest sent/received accounting-relevant data. Enumerations: with-idle-time (1) without-idle-time (2)
WalledStatus
Toggles activation of Walled Garden and of dependent fields WalledNetwork, WalledNetmask, WalledURL, TermsURL. Enumerations: enabled (1) disabled (2)
DefaultLanguage
Default-language used for Web-interface. Range: 3 to 3

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH