>> MIB - Management Information Base
>> Table: ipHostsAliveTable - (.1.3.6.1.4.1.272.4.5.19.1)
Description: This table specifies the watched IP addresses. Entries in the table are created and removed manually by network management.
ipHostsAliveTable
OID | Name | Type | Access
.1 | Group | INTEGER | RW
.2 | IPAddress | IpAddress | RW
.3 | State | ENUM | R
.4 | Interval | INTEGER | RW
.5 | DownAction | ENUM | D
.6 | FirstIfIndex | INTEGER | RW
.7 | Range | INTEGER | RW
.8 | SrcIPAddress | IpAddress | RW
.9 | Trials | INTEGER | RW
Group
The group of the watched IP-Addresses Range: 0 to 255
IPAddress
The watched IP-Address. If set to zero, the default gateway is used.
State
The State of the watched IP-Address Enumerations: alive (1) down (2)
Interval
This is the timeinterval for state verification Range: 1 to 65536
DownAction
This action must be perform, if the hosts do not answer Enumerations: up (1) down (2) delete (3) none (4) reset (5) redial (6)
FirstIfIndex
The first ifc
Range
The range of all ifc's Range: 0 to 65536
SrcIPAddress
The source IP-Address
Trials
How many ping attempts until host is considered down. Default value is 3. Range: 1 to 65535

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH