>> MIB - Management Information Base
>> Table: ipMRoute - (.1.3.6.1.2.1.83.1.1)
ipMRoute
OID | Name | Type | Access
.1 | able | ENUM | RW
.7 | tryCount | Gauge32 | R
able
The enabled status of IP Multicast routing on this router. Enumerations: enabled (1) disabled (2)
tryCount
The number of rows in the ipMRouteTable. This can be used to monitor the multicast routing table size.

MIB Reference to Software Version 7.9.5 generated on 2010/10/07. Provided by webmaster@funkwerk-ec.com Copyright ©2010 by Funkwerk Enterprise Communications GmbH