>> MIB - Management Information Base
>> Table: systemPhoneFunctionKeyTable - (.1.3.6.1.4.1.272.4.64.2.2.1)
Description: This table contains information concerning system phone function key configuration.
systemPhoneFunctionKeyTable
OID | Name | Type | Access
.1 | Index | SystelFunctionKeyIndex | RW
.2 | ModuleIndex | SystelModuleIndex | RW
.3 | Button | SystelFKButtonIndex | RW
.4 | Level | SystelFKLevel | RW
.5 | Description | DisplayString | RW
.6 | Type | ENUM | RW
.7 | MSNPrio | INTEGER | RW
.8 | TargetIndex | SystelTargetIndex | RW
.9 | TargetString | DisplayString | RW
.10 | AdminStatus | ENUM | D
Index
A unique value for each function key of a system phone. Range: 1 to 65535
ModuleIndex
Variable contains the index of the systemPhoneModuleTable as reference. Range: 1 to 65535
Button
Identifier for each function key. Valid range for systemPhoneFKButton for T400 is 1..22. Valid range for systemPhoneFKButton for T500 is 1..30. Range: 1 to 30
Level
Identifier for the (shift) level of each function key. One short press activates level 0 function, double press activates level 1 function. Range: 0 to 1
Description
The variable contains a short description of the key type, which may be printed on the system telephone label. Length: 0 to 20
Type
Specifies type of function key: dial-standard --> standard speed dialing key, dial-dtmf --> dials a DTMF sequence, dial-keypad --> dials a keypad sequence, extension-subscriber --> line key with LED and pickup function for user extension, extension-team --> line key with LED and pickup function for team extension, trunk-line --> trunk line key to establish next call via a configured trunk line, team-log --> log an extension in or out of a team, system-call-announce --> announcement to a choosen extension, system-call-announce-allow --> allow/restrict incoming announcement inquiries, system-call-exchange --> build up a call exchange connection between system phone and choosen extension, system-call-exchange-allow --> allow/restrict incoming call exchange inquiries, boss-boss --> key has to configure on boss system phone to call the secretary (special line key), boss-secretary --> key has to configure on secretary system phone to call the boss (special line key), boss-diversion --> key has to configure on boss system phone to divert incoming calls to secretary's phone, call-forwarding-cfu --> activate/deactivate call forwarding immidiately for a associated extension to a choosen internal number, call-forwarding-cfb --> activate/deactivate call forwarding if busy for a associated extension to a choosen internal number call-forwarding-cfnr --> activate/deactivate call forwarding if no reply for a associated extension to a choosen internal number, macro --> macro key (configuration only via system phone), headset --> prepare a headset call (off-hock) or accept incoming call with headset, auto-accept --> activate/deactivate automatic call accpetance, bundle --> establish next call via a configured bundle, connection --> key to change between two calls (for the correct function of this function key type you have to configure at least two (2) connection keys, to switch between two connections) system-parking --> depositing a subscriber to configured system parking place (open inquiry) or fetch a subscriber of system parking place internal-line-access --> get internal call waiting tone if automatic outside line access is activated hotel-room --> key has to configure on first level of receiption system phone to checkin or checkout hotel rooms agent-time --> key has to configure on first level of agent system phone to activate/deactivate agent time for associated agent night-mode --> activate/deactivate the PBX nightmode (eg. for switching variants of teams, TFE, CoS, etc.) hotel-room-connect --> key is automatically set to second level on system phone if a hotel-room is configured, with a double press the receiption can establish a call to choosen hotel room agent-time-renew --> key is automatically set to second level on system phone if a agent-time is configured, with a double press the agent can renew associated agent timer. do-not-disturb --> activate / deactivate the do not disturb mode of NG system phones (settings for this mode have to modify in systemPhoneFacilityTable shift --> this key have to configure as alternative to the double keypress to get access to the second level function keys. If the shift-key is pressed user get access to the second level functions parallel-ringing --> this key activates or deactivates the parallel ringing option nop --> this key is only a dummy key and leads to no operation in system phone. It is usefull to use this keytype if second level should be locked. Enumerations: dial-standard (1) dial-dtmf (2) dial-keypad (3) extension-subscriber (4) extension-team (5) trunk-line (6) team-log (7) system-call-announce (8) system-call-announce-allow (9) system-call-exchange (10) system-call-exchange-allow (11) boss-boss (12) boss-secretary (13) boss-diversion (14) call-forwarding-cfu (15) call-forwarding-cfb (16) call-forwarding-cfnr (17) macro (18) headset (19) auto-accept (20) bundle (21) connection (22) system-parking (23) internal-line-access (24) hotel-room (25) agent-time (26) night-mode (27) hotel-room-connect (28) agent-time-renew (29) do-not-disturb (30) shift (31) parallel-ringing (32) nop (33)
MSNPrio
This variable contains the index of the selected MSN within the phone, for which this function shall be activated. Only used when selecting the systemPhoneFKType: team-log, call-forwarding-xxx or auto-accept. 1 .. 9 : The function key is attributed to a specific MSN. 0 : The function key is attributed to the default MSN. Range: 0 to 9
TargetIndex
The variable contains either ExtensionIndex, GroupIndex, TrunkGroupIndex, TrunkBundleIndex or SystemNumberPosition, depending upon the function key type selected. Range: 1 to 65535
TargetString
Variable contents depends upon the function key configured. It may be either a dialling number, a DTMF sequence, a keypad sequence, a call forwarding target number or a macro key sequence. Length: 0 to 26
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH