>> MIB - Management Information Base
>> Table: adslAtucPerfDataTable - (.1.3.6.1.4.1.272.4.30.1.1.12.1)
Description: An entry in adslAtucPerfDataTable.
adslAtucPerfDataTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Lofs | INTEGER | R
.3 | Loss | INTEGER | R
.4 | Lprs | INTEGER | R
.5 | ESs | INTEGER | R
.6 | ValidIntervals | INTEGER | R
.7 | InvalidIntervals | INTEGER | R
.8 | Curr15MinTimeElapsed | INTEGER | R
.9 | Curr15MinLofs | INTEGER | R
.10 | Curr15MinLoss | INTEGER | R
.11 | Curr15MinLprs | INTEGER | R
.12 | Curr15MinESs | INTEGER | R
.13 | Curr1DayTimeElapsed | INTEGER | R
.14 | Curr1DayLofs | INTEGER | R
.15 | Curr1DayLoss | INTEGER | R
.16 | Curr1DayLprs | INTEGER | R
.17 | Curr1DayESs | INTEGER | R
.18 | Prev1DayMoniSecs | INTEGER | R
.19 | Prev1DayLofs | INTEGER | R
.20 | Prev1DayLoss | INTEGER | R
.21 | Prev1DayLprs | INTEGER | R
.22 | Prev1DayESs | INTEGER | R
IfIndex
Specifies the ADSL interface index.
Lofs
Count of the number of Loss of Framing failures since agent reset.
Loss
Count of the number of Loss of Signal failures since agent reset.
Lprs
Count of the number of Loss of Power failures since agent reset.
ESs
Count of the number of Errored Seconds since agent reset. The errored second parameter is a count of one-second intervals containing one or more crc anomalies, or one or more los or sef defects.
ValidIntervals
The number of previous 15-minute intervals in the interval table for which data was collected. Given that <n> is the maximum # of intervals supported. The value will be <n> unless the measurement was (re-)started within the last (<n>*15) minutes, in which case the value will be the number of complete 15 minute intervals for which the agent has at least some data. In certain cases (e.g., in the case where the agent is a proxy) it is possible that some intervals are unavailable. In this case, this interval is the maximum interval number for which data is available. Range: 0 to 96
InvalidIntervals
The number of intervals in the range from 0 to the value of adslAtucPerfValidIntervals for which no data is available. This object will typically be zero except in cases where the data for some intervals are not available (e.g., in proxy situations). Range: 0 to 96
Curr15MinTimeElapsed
Total elapsed seconds in this interval. Range: 0 to 899
Curr15MinLofs
Count of seconds in the mandatory 15 minute interval when there was Loss of Framing.
Curr15MinLoss
Count of seconds in the mandatory 15 minute interval when there was Loss of Signal.
Curr15MinLprs
Count of seconds in the mandatory 15 minute interval when there was Loss of Power.
Curr15MinESs
Count of Errored Seconds in the mandatory 15 minute interval. The errored second parameter is a count of one-second intervals containing one or more crc anomalies, or one or more los or sef defects.
Curr1DayTimeElapsed
Number of seconds that have elapsed since the beginning of the mandatory 1-day interval. Range: 0 to 86399
Curr1DayLofs
Count of the number of seconds when there was Loss of Framing during the mandatory day as measured by adslAtucPerfCurr1DayTimeElapsed.
Curr1DayLoss
Count of the number of seconds when there was Loss of Signal during the mandatory day as measured by adslAtucPerfCurr1DayTimeElapsed.
Curr1DayLprs
Count of the number of seconds when there was Loss of Power during the mandatory day as measured by adslAtucPerfCurr1DayTimeElapsed.
Curr1DayESs
Count of Errored Seconds during the mandatory day as measured by adslAtucPerfCurr1DayTimeElapsed. The errored second parameter is a count of one-second intervals containing one or more crc anomalies, or one or more los or sef defects.
Prev1DayMoniSecs
The amount of time in the previous 1-day interval over which the performance monitoring information is actually counted. This value will be the same as the interval duration except in a situation where performance monitoring data could not be collected for any reason. Range: 0 to 86400
Prev1DayLofs
Count of seconds in the interval when there was Loss of Framing within the most recent previous 1-day period.
Prev1DayLoss
Count of seconds in the interval when there was Loss of Signal within the most recent previous 1-day period.
Prev1DayLprs
Count of seconds in the interval when there was Loss of Power within the most recent previous 1-day period.
Prev1DayESs
Count of Errored Seconds within the most recent previous 1-day period. The errored second parameter is a count of one-second intervals containing one or more crc anomalies, or one or more los or sef defects.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH