>> MIB - Management Information Base
>> Table: pimStarGTable - (.1.3.6.1.4.1.272.4.5.54.2.1.4.1)
Description: An entry (conceptual row) in the pimStarGTable.
pimStarGTable
OID | Name | Type | Access
.1 | AddressType | ENUM | R
.2 | GrpAddress | InetAddressIPv6 | R
.3 | UpTime | TimeTicks | R
.4 | PimMode | ENUM | R
.5 | RPAddressType | ENUM | R
.6 | RPAddress | InetAddressIPv6 | R
.7 | PimModeOrigin | ENUM | R
.8 | RPIsLocal | ENUM | R
.9 | UpstreamJoinState | ENUM | R
.10 | UpstreamJoinTimer | TimeTicks | R
.11 | UpstreamNeighborType | ENUM | R
.12 | UpstreamNeighbor | InetAddressIPv6 | R
.13 | RPFIfIndex | InterfaceIndexOrZero | R
.14 | RPFNextHopType | ENUM | R
.15 | RPFNextHop | InetAddressIPv6 | R
.16 | RPFRouteProtocol | ENUM | R
.17 | RPFRouteAddress | InetAddressIPv6 | R
.18 | RPFRoutePrefixLength | InetAddressPrefixLength | R
.19 | RPFRouteMetricPref | Unsigned32 | R
.20 | RPFRouteMetric | Unsigned32 | R
AddressType
The address type of this multicast group. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
GrpAddress
The multicast group address. The InetAddressType is given by the pimStarGAddressType object. Length: 16 to 16
UpTime
The time since this entry was created by the local router.
PimMode
Whether this entry represents an ASM (Any Source Multicast, used with PIM-SM) or BIDIR-PIM group. Enumerations: asm (3) bidir (4)
RPAddressType
The address type of the Rendezvous Point (RP), or unknown(0) if the RP address is unknown. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
RPAddress
The address of the Rendezvous Point (RP) for the group. The InetAddressType is given by the pimStarGRPAddressType. Length: 16 to 16
PimModeOrigin
The mechanism by which the PIM mode and RP for the group were learned. Enumerations: fixed (1) configRp (2) configSsm (3) bsr (4) autoRP (5) embedded (6) other (7)
RPIsLocal
Whether the local router is the RP for the group. Enumerations: true (1) false (2)
UpstreamJoinState
Whether the local router should join the RP tree for the group. This corresponds to the state of the upstream (*,G) state machine in the PIM-SM specification. Enumerations: notJoined (1) joined (2)
UpstreamJoinTimer
The time remaining before the local router next sends a periodic (*,G) Join message on pimStarGRPFIfIndex. This timer is called the (*,G) Upstream Join Timer in the PIM-SM specification. This object is zero if the timer is not running.
UpstreamNeighborType
The primary address type of the upstream neighbor, or unknown(0) if the upstream neighbor address is unknown or is not a PIM neighbor. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
UpstreamNeighbor
The primary address of the neighbor on pimStarGRPFIfIndex that the local router is sending periodic (*,G) Join messages to. The InetAddressType is given by the pimStarGUpstreamNeighborType object. This address is called RPF'(*,G) in the PIM-SM specification. Length: 16 to 16
RPFIfIndex
The value of ifIndex for the RPF interface towards the RP, or zero if the RPF interface is unknown. Range: 0 to 2147483647
RPFNextHopType
The address type of the RPF next hop towards the RP, or unknown(0) if the RPF next hop is unknown. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
RPFNextHop
The address of the RPF next hop towards the RP. The InetAddressType is given by the pimStarGRPFNextHopType object. This address is called MRIB.next_hop(RP(G)) in the PIM-SM specification. Length: 16 to 16
RPFRouteProtocol
The routing mechanism via which the route used to find the RPF interface towards the RP was learned. Enumerations: other (1) local (2) netmgmt (3) icmp (4) egp (5) ggp (6) hello (7) rip (8) isIs (9) esIs (10) ciscoIgrp (11) bbnSpfIgp (12) ospf (13) bgp (14) idpr (15) ciscoEigrp (16) dvmrp (17)
RPFRouteAddress
The IP address which when combined with the corresponding value of pimStarGRPFRoutePrefixLength identifies the route used to find the RPF interface towards the RP. The InetAddressType is given by the pimStarGRPFNextHopType object. This address object is only significant up to pimStarGRPFRoutePrefixLength bits. The remainder of the address bits are zero. Length: 16 to 16
RPFRoutePrefixLength
The prefix length which when combined with the corresponding value of pimStarGRPFRouteAddress identifies the route used to find the RPF interface towards the RP. The InetAddressType is given by the pimStarGRPFNextHopType object. Range: 0 to 2040
RPFRouteMetricPref
The metric preference of the route used to find the RPF interface towards the RP. Range: 0 to 2147483647
RPFRouteMetric
The routing metric of the route used to find the RPF interface towards the RP.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH