>> MIB - Management Information Base
>> Table: ipMRoute - (.1.3.6.1.2.1.83.1.1)
ipMRoute
OID | Name | Type | Access
.1 | Enable | ENUM | RW
.7 | EntryCount | Gauge32 | R
Enable
The enabled status of IP Multicast routing on this router. Enumerations: enabled (1) disabled (2)
EntryCount
The number of rows in the ipMRouteTable. This can be used to monitor the multicast routing table size.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH