>> MIB - Management Information Base
>> Table: isdnCallHistoryTable - (.1.3.6.1.4.1.272.4.2.8.1)
Description: The isdnCallHistoryTable contains information pertaining to the last 20 ISDN calls made, since the last system startup. Each call that appears in the isdnCallTable, will have its information stored here (temporarily), once it disconnects. Creating entries: Entries are added by the system once a call is disconnected. Deleting entries: Entries are removed by the system. The table is designed as a circular queue (or FIFO); the most calls are stored at inx 19 with older calls rolling off the top of the table at inx 00.
isdnCallHistoryTable
OID | Name | Type | Access
.1 | StkNumber | INTEGER | R
.2 | Type | ENUM | R
.3 | Time | Date | R
.4 | Duration | INTEGER | R
.5 | IsdnIfIndex | INTEGER | R
.6 | Channel | INTEGER | R
.7 | DspItem | ENUM | R
.8 | RemoteNumber | DisplayString | R
.9 | RemoteSubaddress | OCTET STRING | R
.10 | LocalNumber | DisplayString | R
.11 | LocalSubaddress | OCTET STRING | R
.12 | ServiceIndicator | ENUM | R
.13 | AddInfo | INTEGER | R
.14 | BC | OCTET STRING | R
.15 | LLC | OCTET STRING | R
.16 | HLC | OCTET STRING | R
.17 | Charge | INTEGER | R
.18 | DSS1Cause | HexValue | R
.19 | 1TR6Cause | HexValue | R
.20 | LocalCause | ENUM | R
.21 | ChargeInfo | DisplayString | R
.22 | Screening | ENUM | R
.23 | Info | DisplayString | R
.24 | ReceivedPackets | Counter32 | R
.25 | ReceivedOctets | Counter32 | R
.26 | ReceivedErrors | Counter32 | R
.27 | TransmitPackets | Counter32 | R
.28 | TransmitOctets | Counter32 | R
.29 | TransmitErrors | Counter32 | R
.30 | ReceiveDiscards | Counter32 | R
.31 | AssociatedIfIndex | INTEGER | R
StkNumber
The number of the ISDN-Stack, this call went through. Range: 0 to 31
Type
The direction of the call, incoming or outgoing. Enumerations: incoming (1) outgoing (2)
Time
The time the call was received (incoming) or was placed (outgoing). Range: 0 to -1
Duration
The duration of the call in seconds.
IsdnIfIndex
The corresponding ISDN interface that this call used.
Channel
The corresponding B-channel on this ISDN interface. Range: 0 to 31
DspItem
The item this call was connected to. Routing tasks (IP, IPX, X.25, bridging, ...) use ppp(1). The isdnlogin program uses login(2). CAPI 1.1 programs, use the items eaz0(48) .. eaz9(57) are used. Enumerations: ppp (1) login (2) undefined (10) ppp-64k (11) ppp-56k (12) ppp-modem (13) ppp-dovb (14) ppp-v110-1200 (15) ppp-v110-2400 (16) ppp-v110-4800 (17) ppp-v110-9600 (18) ppp-v110-14400 (19) ppp-v110-19200 (20) ppp-v110-38400 (21) ppp-x75 (22) ppp-v120 (23) pots (25) ppp-modem-profile-1 (26) ppp-modem-profile-2 (27) ppp-modem-profile-3 (28) ppp-modem-profile-4 (29) ppp-modem-profile-5 (30) ppp-modem-profile-6 (31) ppp-modem-profile-7 (32) ppp-modem-profile-8 (33) ppp-dovb-64k (34) eaz0 (48) eaz1 (49) eaz2 (50) eaz3 (51) eaz4 (52) eaz5 (53) eaz6 (54) eaz7 (55) eaz8 (56) eaz9 (57) x25-pad (58) capi2 (59) ipsec (60) x25 (61) service-call (62)
RemoteNumber
The ISDN number that was called (for outgoing calls) or was calling (for incoming calls). Length: 0 to 255
RemoteSubaddress
The subaddress of the remote number. See isdnCall- HistoryRemoteNumber.
LocalNumber
The calling party number that was sent (with the outgoing call) or was received (with incoming calls). Length: 0 to 255
LocalSubaddress
The subaddress of the calling party number.
ServiceIndicator
Service indicator that was sent on the ISDN D-channel when the call was established. Enumerations: telephony (1) ab-services (2) x21-services (3) fax-group4 (4) btx (5) data-transfer (7) x25-services (8) facsimile64 (9) mixed-mode (10) telecontrol (13) graphics-phone (14) teletex (15) video-phone (16)
AddInfo
Additional information that was sent on the ISDN D-channel when the call was established. Only sent/received when using the 1TR6 protocol. Range: 0 to 255
BC
Bearer Capability that was sent on the ISDN D-channel when the call was established.
LLC
Low Layer Capability that was sent on the ISDN D-channel when the call was established.
HLC
High Layer Capability that was sent on the ISDN D-channel when the call was established.
Charge
The number of charging ticks received for this connection. Actual charges can be computed by multiplying this value with the unit price, e.g. .12 DM in Germany. If you aren't receiving charging information for outgoing calls, verify with your local ISDN provider to make sure this option being provided/is available. As an option, this Object may contain the charge measured in 1/1000 of the respective currency. See also ChargeInfo for textual information.
DSS1Cause
ISDN error condition reported by the DSS1 protocol, for Euro ISDN. See Software Reference Manual. Range: 0 to -1
1TR6Cause
ISDN error condition reported by the 1TR6 protocol, for National ISDN in Germany. See Software Reference Manual. Range: 0 to -1
LocalCause
ISDN error condition reported by the system locally. See Software Reference Manual. Enumerations: unknownprim (1) outstate (2) iemissing (3) ienotallowed (4) look (5) nolink (6) nocallref (7) nomem (8) notready (9) busy (10) chanbusy (11) l3timer (12) l3restart (13) l3error (14) l1error (15) nocontrl (16)
ChargeInfo
Textual information of charge, i.e. 0.12 DM or 3 units Length: 0 to 255
Screening
Screening Indicator of the calling party number of incoming calls. The calling partys number (CPN) may be assigned either by the user placing the call or by the telephone switching station. If the CPN was assigned by the user the switching station may optionally verify the address. indicator: CPN assigned: verification: `user' by user none `user-verified' by user verification successful `user-failed' by user verification failed `network' by network none Enumerations: user (1) user-verified (2) user-failed (3) network (4) undefined (5)
Info
Additional information to identify the call Length: 0 to 255
ReceivedPackets
Count of received valid HDLC Frames.
ReceivedOctets
Count of received valid HDLC Octets.
ReceivedErrors
Count of received invalid HDLC Frames.
TransmitPackets
Count of transmitted HDLC Frames.
TransmitOctets
Count of transmitted Octets.
TransmitErrors
Count of transmit errors (Collision, TX underrun).
ReceiveDiscards
Count of received and discarded data frames.
AssociatedIfIndex
The index of the associated virtual interface.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH