>> MIB - Management Information Base
>> Table: mobileOperatorTable - (.1.3.6.1.4.1.272.4.41.4.1.23.1)
Description: A single mobileOperatorTable entry.
mobileOperatorTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Code | INTEGER | R
.3 | AcT | ENUM | R
.4 | Status | ENUM | R
.5 | Name | DisplayString | R
IfIndex
The index of the corresponding TTY interface.
Code
The PLMN code of the network operator.
AcT
The Access Type the modem actually registers on. Normally the `edge' or `hs*pa' Access Types aren't provided in detail by the network operator and/or modem. Possible Access Types are: unknown(1) gsm(2) -- GSM compact-gsm(3) -- CGSM umts(4) -- UMTS gsm-edge(5) -- GPRS/EDGE umts-hsdpa(6) -- HSDPA umts-hsupa(7) -- HSUPA umts-hspa(8) -- HSPA lte(9) -- LTE hspa-plus(10) -- HSPA+ cdma-rev0(11) -- CDMA 1xEV-DO Rev. 0 cdma-revA(12) -- CDMA 1xEV-DO Rev. A cdma-revB(13) -- CDMA 1xEV-DO Rev. B Enumerations: unknown (1) gsm (2) compact-gsm (3) umts (4) gsm-edge (5) umts-hsdpa (6) umts-hsupa (7) umts-hspa (8) lte (9) hspa-plus (10) cdma-rev0 (11) cdma-revA (12) cdma-revB (13)
Status
The registration status depending on the network operator. The following states can occur: - unknown(1) -- no idea - available(2) -- registration possible - current(3) -- successfully registered - forbidden(4) -- no roaming possible Enumerations: unknown (1) available (2) forbidden (4)
Name
The name of the network operator. Length: 0 to 60

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH