>> MIB - Management Information Base
>> Table: ethIfTable - (.1.3.6.1.4.1.272.4.37.1.1)
Description: The ethIfTable allows to perform interface status changes of one or more interfaces based on a status transition of another interface.
ethIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.4 | PortGroup | INTEGER | RW
.5 | MACSlot | INTEGER | RW
.6 | MACUnit | INTEGER | RW
.7 | AdminStatus | ENUM | RW
Index
A unique value for each interface. Its value ranges between 1000 and the value of ifNumber. The following information is encoded in the ifIndex: a. An ifIndex between 1000 and 9999 define hardware interfaces with the following attributes. b. An ifIndex greater than or equal to 10000 defines a software interface. Examples include the dialup-interfaces as defined in the biboPPPTable.
PortGroup
The port group the interface is member of. Range: 0 to 99
MACSlot
The slot of the connected media access controller. Range: 0 to 9
MACUnit
The unit of the connected media access controller. Range: 0 to 9
AdminStatus
description not available Enumerations: down (1) up (2)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH